(footprint "QFN50P500X500X80-33T310"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "32-QFN, 0.50 mm pitch, 5.00 X 5.00 X 0.80 mm body, 3.10 X 3.10 mm thermal pad\n\n32-pin QFN package with 0.50 mm pitch with body size 5.00 X 5.00 X 0.80 mm and thermal pad size 3.10 X 3.10 mm")
	(property "Reference" "REF**"
		(at 0 -3.5909 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "402288dd-c038-4ab7-a316-bf3315fde71a")
		(effects
			(font
				(size 1.1684 1.1684)
				(thickness 0.1016)
			)
			(justify bottom)
		)
	)
	(property "Value" "QFN50P500X500X80-33T310"
		(at 0 3.5909 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "cb9d17b0-07d5-485b-a604-82b5d1aad3a0")
		(effects
			(font
				(size 1.1684 1.1684)
				(thickness 0.1016)
			)
			(justify top)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "024060b1-9b1e-4e1c-959b-4b34baa8c1cc")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "94f770e6-8304-4ae7-9ac4-c85a934ed5f4")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "f5c9aaf0-2de9-464b-9cb4-061d9ffb708b")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(fp_line
		(start -2.5 -2.5)
		(end -2.139 -2.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "de3b0bac-8428-4424-a54b-71af9cb13a2d")
	)
	(fp_line
		(start -2.5 -2.139)
		(end -2.5 -2.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "eb0c026c-18a4-4e71-83dd-711f7df61570")
	)
	(fp_line
		(start -2.5 2.139)
		(end -2.5 2.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "b2aaf8a9-2a9e-4e6f-94ed-11896507ee2b")
	)
	(fp_line
		(start -2.5 2.5)
		(end -2.139 2.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "8dd68698-6f89-4fa3-be5e-5f1c8455db54")
	)
	(fp_line
		(start 2.5 -2.5)
		(end 2.139 -2.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f3b8793c-4171-40dc-989b-1da6557346b1")
	)
	(fp_line
		(start 2.5 -2.139)
		(end 2.5 -2.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "035d4c47-2bba-46da-a40d-775b278ad185")
	)
	(fp_line
		(start 2.5 2.139)
		(end 2.5 2.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "4d2329ca-dd5b-417c-b3ce-4f88468e600f")
	)
	(fp_line
		(start 2.5 2.5)
		(end 2.139 2.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "57482712-617f-4da3-8f90-706afc064910")
	)
	(fp_circle
		(center -3.004 -2.389)
		(end -2.879 -2.389)
		(stroke
			(width 0.25)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "48ecec73-2abe-48ee-a513-98c8e9a8e413")
	)
	(fp_line
		(start -2.5 -2.5)
		(end 2.5 -2.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "bdfb0b96-d36f-4a9f-9e90-928a14723e37")
	)
	(fp_line
		(start -2.5 2.5)
		(end -2.5 -2.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "9144b5f9-69d7-4940-ab0c-c65196544a8f")
	)
	(fp_line
		(start 2.5 -2.5)
		(end 2.5 2.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "18bf585e-9435-4dcb-b663-847561b550d0")
	)
	(fp_line
		(start 2.5 2.5)
		(end -2.5 2.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b4393f6a-ef03-4845-8997-4a82ee8c5c95")
	)
	(pad "1" smd roundrect
		(at -2.4873 -1.75)
		(size 0.9373 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "4c255201-6dc0-4fe0-882b-f48fee9dcf0e")
	)
	(pad "2" smd roundrect
		(at -2.4873 -1.25)
		(size 0.9373 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "55ac28f7-8581-46cb-bb01-b390e1d77a52")
	)
	(pad "3" smd roundrect
		(at -2.4873 -0.75)
		(size 0.9373 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "11cdeba7-e00b-4bd1-aad5-3562e85278f4")
	)
	(pad "4" smd roundrect
		(at -2.4873 -0.25)
		(size 0.9373 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "15b4be0a-11ee-46e7-a322-f05fb0be38fe")
	)
	(pad "5" smd roundrect
		(at -2.4873 0.25)
		(size 0.9373 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "b67ebed4-bea1-4a85-b959-815a2b77e8ed")
	)
	(pad "6" smd roundrect
		(at -2.4873 0.75)
		(size 0.9373 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "7577c1b4-bc64-41e0-ab9a-6296cbbaf450")
	)
	(pad "7" smd roundrect
		(at -2.4873 1.25)
		(size 0.9373 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "6311cc58-ca95-4a76-9afc-f752ed3fa11c")
	)
	(pad "8" smd roundrect
		(at -2.4873 1.75)
		(size 0.9373 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "ba9d853a-474a-4895-90bf-a2492b77948e")
	)
	(pad "9" smd roundrect
		(at -1.75 2.4873 90)
		(size 0.9373 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "efa9830b-e84e-4aa0-89c2-f0008cb213a7")
	)
	(pad "10" smd roundrect
		(at -1.25 2.4873 90)
		(size 0.9373 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "76e0be4d-b139-4be7-9fb7-1d8bc81a62fa")
	)
	(pad "11" smd roundrect
		(at -0.75 2.4873 90)
		(size 0.9373 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "19f08cef-b2a4-4254-b1f4-bfe57b1f0586")
	)
	(pad "12" smd roundrect
		(at -0.25 2.4873 90)
		(size 0.9373 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "bc0562d7-e546-4f01-a568-b35806a58ab8")
	)
	(pad "13" smd roundrect
		(at 0.25 2.4873 90)
		(size 0.9373 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "98b62852-0ecb-46d8-b7a3-5397fc5e7c26")
	)
	(pad "14" smd roundrect
		(at 0.75 2.4873 90)
		(size 0.9373 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "ba7c91fa-c533-4a4f-9493-2bc91714a1df")
	)
	(pad "15" smd roundrect
		(at 1.25 2.4873 90)
		(size 0.9373 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "8162187c-22be-4532-abbd-e206f88416a2")
	)
	(pad "16" smd roundrect
		(at 1.75 2.4873 90)
		(size 0.9373 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "abe772c8-b873-4340-a8e7-d58555f1afab")
	)
	(pad "17" smd roundrect
		(at 2.4873 1.75)
		(size 0.9373 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "53bec245-7f09-4e8f-ae40-ec551aae595b")
	)
	(pad "18" smd roundrect
		(at 2.4873 1.25)
		(size 0.9373 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "7daad39f-17cf-40fc-ba89-91468afc400a")
	)
	(pad "19" smd roundrect
		(at 2.4873 0.75)
		(size 0.9373 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "bf34dc2e-e345-4002-81a8-d72174fc0f30")
	)
	(pad "20" smd roundrect
		(at 2.4873 0.25)
		(size 0.9373 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "a8d892b1-5ad4-44f8-8a4f-a7730d5f120a")
	)
	(pad "21" smd roundrect
		(at 2.4873 -0.25)
		(size 0.9373 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "69962d38-fc2a-4cd8-bde6-8f71ec02ff86")
	)
	(pad "22" smd roundrect
		(at 2.4873 -0.75)
		(size 0.9373 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "b29fcb2e-4750-4f00-a86e-76bdef210c0e")
	)
	(pad "23" smd roundrect
		(at 2.4873 -1.25)
		(size 0.9373 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "c43d2b50-33f0-47a6-9eb8-07dea6c33a54")
	)
	(pad "24" smd roundrect
		(at 2.4873 -1.75)
		(size 0.9373 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "793836bb-b2c9-4a93-8f1a-a35fbd807980")
	)
	(pad "25" smd roundrect
		(at 1.75 -2.4873 90)
		(size 0.9373 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "d3f4d1cf-7dce-4d8a-966a-fe2cd5ef7a6e")
	)
	(pad "26" smd roundrect
		(at 1.25 -2.4873 90)
		(size 0.9373 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "4f0ee44f-2234-4768-ae07-5eba889affc7")
	)
	(pad "27" smd roundrect
		(at 0.75 -2.4873 90)
		(size 0.9373 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "e3a89c21-ccff-4465-a475-b6ebd155330a")
	)
	(pad "28" smd roundrect
		(at 0.25 -2.4873 90)
		(size 0.9373 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "9e37d8c9-8299-468f-9aad-e644aa306cec")
	)
	(pad "29" smd roundrect
		(at -0.25 -2.4873 90)
		(size 0.9373 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "62c3c0d1-9c9e-4abe-bd17-9de50898a48f")
	)
	(pad "30" smd roundrect
		(at -0.75 -2.4873 90)
		(size 0.9373 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "a62647ce-ada1-48a2-9df2-2aed226d4029")
	)
	(pad "31" smd roundrect
		(at -1.25 -2.4873 90)
		(size 0.9373 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "91ffcd70-113d-41d0-aeec-da0847dde4be")
	)
	(pad "32" smd roundrect
		(at -1.75 -2.4873 90)
		(size 0.9373 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "715dac86-784b-4e09-8d59-5b5c5df1fd9d")
	)
	(pad "33" smd rect
		(at 0 0)
		(size 3.1 3.1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(zone_connect 2)
		(thermal_bridge_angle 0)
		(uuid "f22e327f-6de5-420c-8936-71dc2145a88a")
	)
)