(footprint "SON50P300X300X90-13T170X240N"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "12-SON (DFN), 0.50 mm pitch, 3.00 X 3.00 X 0.90 mm body, 2.40 X 1.70 mm thermal pad\n\n12-pin SON (DFN) package with 0.50 mm pitch with body size 3.00 X 3.00 X 0.90 mm and thermal pad size 2.40 X 1.70 mm")
	(property "Reference" "REF**"
		(at 0 -2.764 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "9ae87bb7-e04f-48d9-b596-4cf9ddb7e706")
		(effects
			(font
				(size 1.1684 1.1684)
				(thickness 0.1016)
			)
			(justify bottom)
		)
	)
	(property "Value" "SON50P300X300X90-13T170X240N"
		(at 0 2.324 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "cbaa03b4-4744-4744-89b6-46633ac922bc")
		(effects
			(font
				(size 1.1684 1.1684)
				(thickness 0.1016)
			)
			(justify top)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "55740118-5ad1-4148-a728-23e483e67eb3")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "457e623f-d310-4749-8ca8-08da6553bae2")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "47e5859f-93cf-4242-bdc1-2a815e8c876a")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(fp_line
		(start -1.5 -1.689)
		(end 1.5 -1.689)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "5a3d3f12-6a8e-48c2-8848-fb22cf7bd788")
	)
	(fp_line
		(start -1.5 1.689)
		(end 1.5 1.689)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2c911348-0f45-4ee1-9fc5-d90bac286a38")
	)
	(fp_circle
		(center -2.004 -1.879)
		(end -1.879 -1.879)
		(stroke
			(width 0.25)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "5e9706da-b3e1-4c09-a7f4-0ed6f811ba19")
	)
	(fp_line
		(start -1.5 -1.5)
		(end 1.5 -1.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "82f3c87b-4887-4570-97b1-51d3c6864739")
	)
	(fp_line
		(start -1.5 1.5)
		(end -1.5 -1.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "699d9481-53ee-4cab-8b3b-f1010a48bd2c")
	)
	(fp_line
		(start 1.5 -1.5)
		(end 1.5 1.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "d2b373e5-b83b-45ac-8298-9c5d2a49fd56")
	)
	(fp_line
		(start 1.5 1.5)
		(end -1.5 1.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "7696598f-9e99-4e14-925c-cb88ef856a62")
	)
	(pad "1" smd roundrect
		(at -1.4506 -1.25)
		(size 0.8107 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "6d2031a0-689c-4820-b8b6-f6e68db2a9d3")
	)
	(pad "2" smd roundrect
		(at -1.4506 -0.75)
		(size 0.8107 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "119322bc-e233-4e15-940a-2a78b404abe5")
	)
	(pad "3" smd roundrect
		(at -1.4506 -0.25)
		(size 0.8107 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "60222c09-f1d0-4cf2-adf2-2d809629ba2c")
	)
	(pad "4" smd roundrect
		(at -1.4506 0.25)
		(size 0.8107 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "af3fdce7-2802-4ebb-b147-9516177623b5")
	)
	(pad "5" smd roundrect
		(at -1.4506 0.75)
		(size 0.8107 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "41a4df2d-8b91-43d6-a393-f64745d2664d")
	)
	(pad "6" smd roundrect
		(at -1.4506 1.25)
		(size 0.8107 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "fda9841d-96cd-4192-b550-f845376dcfaf")
	)
	(pad "7" smd roundrect
		(at 1.4506 1.25)
		(size 0.8107 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "19419ff0-7950-4ea2-91b3-8906873d19d5")
	)
	(pad "8" smd roundrect
		(at 1.4506 0.75)
		(size 0.8107 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "96a64de4-3cf3-429a-8057-f5fb79b45a5d")
	)
	(pad "9" smd roundrect
		(at 1.4506 0.25)
		(size 0.8107 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "b2343f49-1c38-4381-a78b-f8d548fa3982")
	)
	(pad "10" smd roundrect
		(at 1.4506 -0.25)
		(size 0.8107 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "44cf80b6-21de-4d2c-9983-58363f51407a")
	)
	(pad "11" smd roundrect
		(at 1.4506 -0.75)
		(size 0.8107 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "b0a25dd7-3673-4fde-bbe6-e8bffef05b2f")
	)
	(pad "12" smd roundrect
		(at 1.4506 -1.25)
		(size 0.8107 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "8ec3c112-df9d-4d6f-ab9e-cec775b34f2c")
	)
	(pad "13" smd rect
		(at 0 0)
		(size 1.7 2.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(zone_connect 2)
		(thermal_bridge_angle 0)
		(uuid "d83fbfdb-eb1a-48e3-85b7-d5ccbe7c6c18")
	)
)