(footprint "QFN50P400X400X75-21T206"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "20-QFN, 0.50 mm pitch, 4.00 X 4.00 X 0.75 mm body, 2.06 X 2.06 mm thermal pad\n\n20-pin QFN package with 0.50 mm pitch with body size 4.00 X 4.00 X 0.75 mm and thermal pad size 2.06 X 2.06 mm")
	(property "Reference" "REF**"
		(at 0 -2.9909 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "95e11fff-c651-43ef-b5ec-4d2d8542d609")
		(effects
			(font
				(size 1.1684 1.1684)
				(thickness 0.1016)
			)
			(justify bottom)
		)
	)
	(property "Value" "QFN50P400X400X75-21T206"
		(at 0 2.9909 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "9a6f1964-21f0-420a-bc61-585f54a9a13d")
		(effects
			(font
				(size 1.1684 1.1684)
				(thickness 0.1016)
			)
			(justify top)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "ca418534-096c-492d-ac95-7c1ff840aa4a")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "54aeabc6-825b-4efd-8e62-f191f27f980c")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "bb61c310-bc0a-4bc3-9d60-e2650acde530")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(fp_line
		(start -2 -2)
		(end -1.3949 -2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "909fdd63-8ae8-45f0-8707-8097851a3bc4")
	)
	(fp_line
		(start -2 -1.3949)
		(end -2 -2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "cd40a8f2-bd00-44c7-a44c-db1ecc6a2578")
	)
	(fp_line
		(start -2 1.3949)
		(end -2 2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "44d8e501-a785-4b07-b868-b2f3a548a7a6")
	)
	(fp_line
		(start -2 2)
		(end -1.3949 2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "251f772d-746c-4127-b3dd-c78b0e24aed4")
	)
	(fp_line
		(start 2 -2)
		(end 1.3949 -2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ade560c3-c69c-486d-bbec-c3de02b0dee4")
	)
	(fp_line
		(start 2 -1.3949)
		(end 2 -2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "21c471bd-24bb-4b93-ac13-7e7b1f9c5d32")
	)
	(fp_line
		(start 2 1.3949)
		(end 2 2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "b44baa2c-6931-4bc4-b98f-13db05bebdda")
	)
	(fp_line
		(start 2 2)
		(end 1.3949 2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "faf19100-6fd9-4768-888a-83ed4243307e")
	)
	(fp_circle
		(center -2.504 -1.6449)
		(end -2.379 -1.6449)
		(stroke
			(width 0.25)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "3d91ce77-e741-4083-b207-2a8ffb7b6430")
	)
	(fp_line
		(start -2 -2)
		(end 2 -2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "1572ed78-ca76-411f-9c0d-ab18b140185c")
	)
	(fp_line
		(start -2 2)
		(end -2 -2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "9f59af10-b8a8-46a7-be9d-c9c822434eff")
	)
	(fp_line
		(start 2 -2)
		(end 2 2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "847d684c-2d4e-471a-a140-18a9d6d8265a")
	)
	(fp_line
		(start 2 2)
		(end -2 2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "14e2fc89-df17-401c-b1a1-e11073c2f028")
	)
	(pad "1" smd roundrect
		(at -1.875 -1)
		(size 0.9618 0.2818)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "70fea837-46ee-42b2-8e8a-350285265b43")
	)
	(pad "2" smd roundrect
		(at -1.875 -0.5)
		(size 0.9618 0.2818)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "a3563662-77f2-4c88-a425-3a22659ded60")
	)
	(pad "3" smd roundrect
		(at -1.875 0)
		(size 0.9618 0.2818)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "0f2a2c48-366c-4bd1-ae9c-67acc1946112")
	)
	(pad "4" smd roundrect
		(at -1.875 0.5)
		(size 0.9618 0.2818)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "3547b787-ed8f-41b0-af8c-eda7eb3fe7b2")
	)
	(pad "5" smd roundrect
		(at -1.875 1)
		(size 0.9618 0.2818)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "442b325e-2444-4fe3-b085-8fdf79c9e920")
	)
	(pad "6" smd roundrect
		(at -1 1.875 90)
		(size 0.9618 0.2818)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "4ebcedf2-2cce-4c8f-8692-d6f45fda803e")
	)
	(pad "7" smd roundrect
		(at -0.5 1.875 90)
		(size 0.9618 0.2818)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "7fb9cb9a-89f2-43dd-b463-09738bcb1ac1")
	)
	(pad "8" smd roundrect
		(at 0 1.875 90)
		(size 0.9618 0.2818)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "ae2cd54e-8eb4-48a8-a8d7-1d04f737dcdc")
	)
	(pad "9" smd roundrect
		(at 0.5 1.875 90)
		(size 0.9618 0.2818)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "2e48637a-5824-4fa9-a52f-114a6cd61edd")
	)
	(pad "10" smd roundrect
		(at 1 1.875 90)
		(size 0.9618 0.2818)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "9dcaaaf4-7371-4b5c-b62f-59930afa6019")
	)
	(pad "11" smd roundrect
		(at 1.875 1)
		(size 0.9618 0.2818)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "a6fff729-557f-439b-b33c-ccca891dd1b9")
	)
	(pad "12" smd roundrect
		(at 1.875 0.5)
		(size 0.9618 0.2818)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "6680396c-b234-46de-a171-5321577d2ebc")
	)
	(pad "13" smd roundrect
		(at 1.875 0)
		(size 0.9618 0.2818)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "6d0ef0b9-6680-4e28-b89e-5866f434523a")
	)
	(pad "14" smd roundrect
		(at 1.875 -0.5)
		(size 0.9618 0.2818)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "2bff5f6b-fee9-4d97-9c09-7a7153d16e22")
	)
	(pad "15" smd roundrect
		(at 1.875 -1)
		(size 0.9618 0.2818)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "a67ba987-d09a-4b4b-8c9d-198eee11d9e9")
	)
	(pad "16" smd roundrect
		(at 1 -1.875 90)
		(size 0.9618 0.2818)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "c7ad10f1-bb0c-449f-85f0-b9f0d7089e1b")
	)
	(pad "17" smd roundrect
		(at 0.5 -1.875 90)
		(size 0.9618 0.2818)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "1499bd4d-3c1e-47bc-8a8a-c61a7273f788")
	)
	(pad "18" smd roundrect
		(at 0 -1.875 90)
		(size 0.9618 0.2818)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "a083b27c-dd9c-43dd-9326-380008c5a4e6")
	)
	(pad "19" smd roundrect
		(at -0.5 -1.875 90)
		(size 0.9618 0.2818)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "b5c09fcf-a603-4f10-8ee2-4b0e1398a3c9")
	)
	(pad "20" smd roundrect
		(at -1 -1.875 90)
		(size 0.9618 0.2818)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "c921f74c-61b5-49a0-9bdd-843081956fb0")
	)
	(pad "21" smd rect
		(at 0 0)
		(size 2.06 2.06)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(zone_connect 2)
		(thermal_bridge_angle 0)
		(uuid "cc9d834c-067c-439c-8600-f84a431b1797")
	)
)