(footprint "SON50P400X500X80-17T260X400N"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "16-SON (DFN), 0.50 mm pitch, 5.00 X 4.00 X 0.80 mm body, 4.00 X 2.60 mm thermal pad\n\n16-pin SON (DFN) package with 0.50 mm pitch with body size 5.00 X 4.00 X 0.80 mm and thermal pad size 4.00 X 2.60 mm")
	(property "Reference" "REF**"
		(at 0 -3.274 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "f8289cfb-4a2b-4df4-a189-8fed4e0fae51")
		(effects
			(font
				(size 1.1684 1.1684)
				(thickness 0.1016)
			)
			(justify bottom)
		)
	)
	(property "Value" "SON50P400X500X80-17T260X400N"
		(at 0 3.185 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "ebc60461-555e-40f8-b010-c2cc617b3d9e")
		(effects
			(font
				(size 1.1684 1.1684)
				(thickness 0.1016)
			)
			(justify top)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "41a343d3-768a-41fe-8e36-8e040659d3b2")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "93664deb-a7fc-4be1-9456-b6ecf815a585")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "4964ab06-0704-4059-aade-72c868127631")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(fp_line
		(start -2.05 -2.55)
		(end 2.05 -2.55)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "8f743757-369c-4acb-bb2f-3de35d6b6f8a")
	)
	(fp_line
		(start -2.05 -2.139)
		(end -2.05 -2.55)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "4b1c2bbe-bfef-4226-b02d-f0b1d7adecdc")
	)
	(fp_line
		(start -2.05 2.139)
		(end -2.05 2.55)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c8f5109c-fb43-405d-88fa-c171da2deeec")
	)
	(fp_line
		(start -2.05 2.55)
		(end 2.05 2.55)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0cf42f87-7b19-4676-8115-2a21347b8b04")
	)
	(fp_line
		(start 2.05 -2.55)
		(end 2.05 -2.139)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "9a03b182-56d9-406c-90bd-b944885b9c12")
	)
	(fp_line
		(start 2.05 2.55)
		(end 2.05 2.139)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "5c9d1ef1-5ca2-4585-9be3-514d6aa85091")
	)
	(fp_circle
		(center -2.554 -2.389)
		(end -2.429 -2.389)
		(stroke
			(width 0.25)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "2df8c099-bc2b-4725-86dd-60e7971e825a")
	)
	(fp_line
		(start -2.05 -2.55)
		(end 2.05 -2.55)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "a35e2c3e-b967-4bfc-8de7-53891bb3a304")
	)
	(fp_line
		(start -2.05 2.55)
		(end -2.05 -2.55)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "1bbbee5d-36c2-4063-a25b-630deb5de54d")
	)
	(fp_line
		(start 2.05 -2.55)
		(end 2.05 2.55)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "fadb0b2b-f5dd-4812-afe0-0011bc03d864")
	)
	(fp_line
		(start 2.05 2.55)
		(end -2.05 2.55)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "43b75e58-03fc-4b8a-b6a1-8c442d85bbb3")
	)
	(pad "1" smd roundrect
		(at -1.9346 -1.75)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "3de0a6b9-e59a-4c4a-8403-f61ecfc6d9c7")
	)
	(pad "2" smd roundrect
		(at -1.9346 -1.25)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "5dd941a9-7d54-4e08-99f5-215549879cc3")
	)
	(pad "3" smd roundrect
		(at -1.9346 -0.75)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "ea0c4fe7-dbef-4a3e-b4a9-0eed451a9072")
	)
	(pad "4" smd roundrect
		(at -1.9346 -0.25)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "765f6945-b9f6-40f3-9d79-4518387d551f")
	)
	(pad "5" smd roundrect
		(at -1.9346 0.25)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "2f0aa02f-283b-4d40-823c-8d3354372fa9")
	)
	(pad "6" smd roundrect
		(at -1.9346 0.75)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "69cdc952-555b-4c14-8365-daed6c7bf410")
	)
	(pad "7" smd roundrect
		(at -1.9346 1.25)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "449b2d45-c8f1-4879-8991-5bab96e6bea3")
	)
	(pad "8" smd roundrect
		(at -1.9346 1.75)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "8c19c2c9-38cb-4718-a25c-9f7ad5e671f0")
	)
	(pad "9" smd roundrect
		(at 1.9346 1.75)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "bd5918ad-988b-422f-860b-00ad5b161ff7")
	)
	(pad "10" smd roundrect
		(at 1.9346 1.25)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "9d7e5e5c-e7a6-4461-b40e-767a1d1a66f1")
	)
	(pad "11" smd roundrect
		(at 1.9346 0.75)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "b9b57192-a2f0-4568-bd9c-ab7ec7ec8f57")
	)
	(pad "12" smd roundrect
		(at 1.9346 0.25)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "96c2c27d-0653-4eed-bfee-cdb402d3aa0e")
	)
	(pad "13" smd roundrect
		(at 1.9346 -0.25)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "b73ef32e-a831-4bcc-a57e-0ff9565ed20d")
	)
	(pad "14" smd roundrect
		(at 1.9346 -0.75)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "3b9d5a38-1161-492f-8fd0-56d5159a8df4")
	)
	(pad "15" smd roundrect
		(at 1.9346 -1.25)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "35ffc5ae-7e82-4352-8d6f-12d54edb1eff")
	)
	(pad "16" smd roundrect
		(at 1.9346 -1.75)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "5ad3ade9-0dc9-4317-93a1-9e1b1b2e569e")
	)
	(pad "17" smd rect
		(at 0 0)
		(size 2.6 4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(zone_connect 2)
		(thermal_bridge_angle 0)
		(uuid "029c094a-231c-4575-b782-7b691aad2e05")
	)
)