(footprint "Oscillator_SMD_ECS_20CSMV4_2.0x1.6mm"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Miniature Crystal Clock Oscillator ECS 2520MV series, https://www.ecsxtal.com/store/pdf/ECS-2520MV.pdf")
	(tags "Miniature Crystal Clock Oscillator ECS 2520MV series SMD SMT HCMOS")
	(property "Reference" "REF**"
		(at 0 -2.5 0)
		(layer "F.SilkS")
		(uuid "b2b79353-611f-43d1-91fb-95bbce7523af")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "Oscillator_SMD_ECS_20CSMV4_2.0x1.6mm"
		(at 0 2.5 0)
		(layer "F.Fab")
		(uuid "639e41da-2de6-419c-81c3-bf7f25686ccb")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "c33ef51a-4a99-4801-94ee-a3eb8ead8760")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "884d2cc6-412a-4522-9497-90cee957a201")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "6dcb2bd5-e2a7-437f-b043-0a8004289cef")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -0.9 0.32)
		(end -0.9 -0.32)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "69f6c69b-e40e-45f8-9d87-53841f41772f")
	)
	(fp_line
		(start -0.17 1.36)
		(end 0.17 1.36)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ec66d435-2622-4822-9d87-15c77c1559e7")
	)
	(fp_line
		(start -0.16 -1.36)
		(end 0.17 -1.36)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "9aeb0d72-340a-47d3-a8c6-db879ac0474c")
	)
	(fp_line
		(start 0.9 0.32)
		(end 0.9 -0.32)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "689ce109-68de-4f68-8ba5-8ff35dc934c4")
	)
	(fp_circle
		(center -1.1 -1.5)
		(end -1 -1.6)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "e47aa905-a6f8-4b41-a12c-70d69e187f6f")
	)
	(fp_line
		(start -1.1 -1.3)
		(end -1.1 1.3)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "792c3c1f-0208-46b6-8062-176b3de6867a")
	)
	(fp_line
		(start -1.1 -1.3)
		(end 1.1 -1.3)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "20578b83-b35f-4364-8a1f-da29da068217")
	)
	(fp_line
		(start -1.1 1.3)
		(end 1.1 1.3)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "04e49102-e4ca-4fac-8e9a-d93526257fe0")
	)
	(fp_line
		(start 1.1 -1.3)
		(end 1.1 1.3)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "7f41f6b7-8639-4f50-a344-214300c9f2f6")
	)
	(fp_line
		(start -0.8 -0.5)
		(end -0.8 1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "693bfb8d-65ae-48dc-88fb-46b96377b721")
	)
	(fp_line
		(start -0.8 -0.5)
		(end -0.3 -1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "364cc372-fd0a-47e7-bb70-eb0a35c5dd4e")
	)
	(fp_line
		(start -0.8 1)
		(end 0.8 1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "6e8b6746-4cc4-4c35-91c1-123de77f9b03")
	)
	(fp_line
		(start -0.3 -1)
		(end 0.8 -1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "d8760ca9-370b-4bc5-a82c-677274f10055")
	)
	(fp_line
		(start 0.8 -1)
		(end 0.8 1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "22ded5e9-d635-4432-ad06-636136105a90")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
		(uuid "72235894-1a76-4ff1-bfb0-71ffe329257f")
		(effects
			(font
				(size 0.5 0.5)
				(thickness 0.075)
			)
		)
	)
	(pad "1" smd roundrect
		(at -0.6125 -0.91)
		(size 0.825 0.63)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "1c941a22-3171-4d7a-b730-a151bde7ede0")
	)
	(pad "2" smd roundrect
		(at -0.6125 0.91)
		(size 0.825 0.63)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "9a292f7b-cb1b-4920-a7db-2befab82a7cb")
	)
	(pad "3" smd roundrect
		(at 0.6125 0.91)
		(size 0.825 0.63)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "ea7b0b9f-cfa7-4427-90f1-a3d31052f9a2")
	)
	(pad "4" smd roundrect
		(at 0.6125 -0.91)
		(size 0.825 0.63)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "1d6613e4-7b93-4cd3-bea1-8f2ffac3976a")
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(uuid "241b6bdc-f829-43f1-86ff-c34d9f1a086f")
		(name "noGND")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias not_allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -0.9 -1.2) (xy 0.9 -1.2) (xy 0.9 1.2) (xy -0.9 1.2)
			)
		)
	)
	(model "${KICAD8_3DMODEL_DIR}/Oscillator.3dshapes/Oscillator_SMD_ECS_2520MV-xxx-xx-4Pin_2.5x2.0mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)