(footprint "QFN50P400X400X90-21T270N"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "20-QFN, 0.50 mm pitch, 4.00 X 4.00 X 0.90 mm body, 2.70 X 2.70 mm thermal pad\n\n20-pin QFN package with 0.50 mm pitch with body size 4.00 X 4.00 X 0.90 mm and thermal pad size 2.70 X 2.70 mm")
	(property "Reference" "REF**"
		(at 0 -2.9996 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "9c6eea6a-716d-4278-b3e9-597cebd8a05b")
		(effects
			(font
				(size 1.1684 1.1684)
				(thickness 0.1016)
			)
			(justify bottom)
		)
	)
	(property "Value" "QFN50P400X400X90-21T270N"
		(at 0 2.9996 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "bb162722-4381-4028-a833-d4a3faa58c25")
		(effects
			(font
				(size 1.1684 1.1684)
				(thickness 0.1016)
			)
			(justify top)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "329aea17-3c27-4088-8e7e-dfaa6ab3f026")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "15aa94f1-3767-4f30-8940-3a6968432b99")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "e55cc59d-9e80-4b3a-a60e-a25be4cada49")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(fp_line
		(start -2.05 -2.05)
		(end -1.389 -2.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "d68e5149-4f67-40d7-9dfa-d7bddcaa97d7")
	)
	(fp_line
		(start -2.05 -1.389)
		(end -2.05 -2.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c0d6181e-22a6-4c70-97ae-84375e309ae0")
	)
	(fp_line
		(start -2.05 1.389)
		(end -2.05 2.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "18ce3fbe-36de-485c-8e77-07e8a341ddbe")
	)
	(fp_line
		(start -2.05 2.05)
		(end -1.389 2.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "b5f72ed5-a8fc-429e-8770-6869dac44fec")
	)
	(fp_line
		(start 2.05 -2.05)
		(end 1.389 -2.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f2c1a854-471f-4cd8-89f5-d7206a86f714")
	)
	(fp_line
		(start 2.05 -1.389)
		(end 2.05 -2.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "32f74294-3dbf-498d-bb6f-8458a85be2b7")
	)
	(fp_line
		(start 2.05 1.389)
		(end 2.05 2.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "97d43c59-c2cc-4aa2-ba30-39a1b3a2d3cf")
	)
	(fp_line
		(start 2.05 2.05)
		(end 1.389 2.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ddd05a88-6764-4211-b8bc-a7835b7c846d")
	)
	(fp_circle
		(center -2.554 -1.639)
		(end -2.429 -1.639)
		(stroke
			(width 0.25)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "3f9749ce-4bd3-4fb8-aaab-6b9dbeaad08e")
	)
	(fp_line
		(start -2.05 -2.05)
		(end 2.05 -2.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "0a7f8fb5-8ed1-4aa7-8963-50a035e7a192")
	)
	(fp_line
		(start -2.05 2.05)
		(end -2.05 -2.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8deb9d2f-da58-4164-b93a-2866df492c5e")
	)
	(fp_line
		(start 2.05 -2.05)
		(end 2.05 2.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "03718de2-8da2-4c7e-a2ba-4de744e7671c")
	)
	(fp_line
		(start 2.05 2.05)
		(end -2.05 2.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c18f253c-4d2e-420b-92ce-c4dbb09ff499")
	)
	(pad "1" smd roundrect
		(at -1.9456 -1)
		(size 0.838 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "3c92feb8-7726-4e0e-a7ef-7e011263e028")
	)
	(pad "2" smd roundrect
		(at -1.9456 -0.5)
		(size 0.838 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "5d8b188b-367a-4abc-a823-0058cc84bab4")
	)
	(pad "3" smd roundrect
		(at -1.9456 0)
		(size 0.838 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "791c82e0-dbcf-4766-95d5-683e6922f8f4")
	)
	(pad "4" smd roundrect
		(at -1.9456 0.5)
		(size 0.838 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "b269ce38-a109-4b55-b256-107e9fcb0baf")
	)
	(pad "5" smd roundrect
		(at -1.9456 1)
		(size 0.838 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "2ed4eb6a-1862-4f7d-8bd2-79a91fc9cc07")
	)
	(pad "6" smd roundrect
		(at -1 1.9456 90)
		(size 0.838 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "1de02c68-0d41-4ae2-a3a0-f72723195d1e")
	)
	(pad "7" smd roundrect
		(at -0.5 1.9456 90)
		(size 0.838 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "db33c182-165f-4516-9c3a-50b16e2d4f0e")
	)
	(pad "8" smd roundrect
		(at 0 1.9456 90)
		(size 0.838 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "1833c310-dc42-4f7f-9590-726c22c4c97d")
	)
	(pad "9" smd roundrect
		(at 0.5 1.9456 90)
		(size 0.838 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "7c582fa6-8c4e-49af-aad1-a41886385fdc")
	)
	(pad "10" smd roundrect
		(at 1 1.9456 90)
		(size 0.838 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "ebec8de3-b21f-4cbe-a017-cfe3010809d1")
	)
	(pad "11" smd roundrect
		(at 1.9456 1)
		(size 0.838 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "84631ac8-ef9c-40e7-bff2-4240670624b4")
	)
	(pad "12" smd roundrect
		(at 1.9456 0.5)
		(size 0.838 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "bb708360-ba71-4778-b000-be82c18bf99f")
	)
	(pad "13" smd roundrect
		(at 1.9456 0)
		(size 0.838 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "dd82fa8c-2cf9-4cc6-84d2-ae989742f2c8")
	)
	(pad "14" smd roundrect
		(at 1.9456 -0.5)
		(size 0.838 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "ad0e58f9-7d1d-41e2-b10e-5afae567871a")
	)
	(pad "15" smd roundrect
		(at 1.9456 -1)
		(size 0.838 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "937df867-63c4-419f-a5fb-989a3f949efa")
	)
	(pad "16" smd roundrect
		(at 1 -1.9456 90)
		(size 0.838 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "17eccb94-af37-471b-ba24-b94ba758b455")
	)
	(pad "17" smd roundrect
		(at 0.5 -1.9456 90)
		(size 0.838 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "df22c659-a976-4edb-a186-673d96d4f060")
	)
	(pad "18" smd roundrect
		(at 0 -1.9456 90)
		(size 0.838 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "d31c1730-dfe6-40d4-9142-154513a0bbe6")
	)
	(pad "19" smd roundrect
		(at -0.5 -1.9456 90)
		(size 0.838 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "9b97cbc5-b3d0-40c2-b782-1e8cd3d038b4")
	)
	(pad "20" smd roundrect
		(at -1 -1.9456 90)
		(size 0.838 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "2e68ff19-022f-479e-b12d-8a12fbc928e3")
	)
	(pad "21" smd rect
		(at 0 0)
		(size 2.7 2.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(zone_connect 2)
		(thermal_bridge_angle 0)
		(uuid "b8a1f21c-9d13-4a7a-be68-ab2d507e6855")
	)
)