(footprint "QFN50P400X400X75-25T270"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "24-QFN, 0.50 mm pitch, 4.00 X 4.00 X 0.75 mm body, 2.70 X 2.70 mm thermal pad\n\n24-pin QFN package with 0.50 mm pitch with body size 4.00 X 4.00 X 0.75 mm and thermal pad size 2.70 X 2.70 mm")
	(property "Reference" "REF**"
		(at 0 -3.0996 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "e5d875f6-127c-4a1e-93e7-a8abdb803842")
		(effects
			(font
				(size 1.1684 1.1684)
				(thickness 0.1016)
			)
			(justify bottom)
		)
	)
	(property "Value" "QFN50P400X400X75-25T270"
		(at 0 3.0996 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "71515ea5-f2c9-483c-91f3-d6fcec17227f")
		(effects
			(font
				(size 1.1684 1.1684)
				(thickness 0.1016)
			)
			(justify top)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "d5d2b3c6-d796-4e72-8223-600648f890dc")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "17d816c2-a723-4bca-ad62-ffcb02f8852b")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "2ca379bd-dcf9-44e5-ad84-d5c38490954c")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(fp_line
		(start -2.05 -2.05)
		(end -1.639 -2.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "1ce494bf-f18f-4d95-baf9-5c7f8dc04d02")
	)
	(fp_line
		(start -2.05 -1.639)
		(end -2.05 -2.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e2e04906-57fa-47e8-a6b4-b6968cf36ada")
	)
	(fp_line
		(start -2.05 1.639)
		(end -2.05 2.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "19434142-9a03-4e5e-832d-e3770c0c0aab")
	)
	(fp_line
		(start -2.05 2.05)
		(end -1.639 2.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "a1f0856d-d0e0-429a-af2d-a4c73514df14")
	)
	(fp_line
		(start 2.05 -2.05)
		(end 1.639 -2.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "457f8302-880c-491a-bea9-feaa34ca1453")
	)
	(fp_line
		(start 2.05 -1.639)
		(end 2.05 -2.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "8452f3e0-91f8-42c1-b0da-bf1891909894")
	)
	(fp_line
		(start 2.05 1.639)
		(end 2.05 2.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "47499a69-312c-4f41-98c5-acb384d192cc")
	)
	(fp_line
		(start 2.05 2.05)
		(end 1.639 2.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "68193ec2-3807-4e07-b907-bc1526efa789")
	)
	(fp_circle
		(center -2.554 -1.889)
		(end -2.429 -1.889)
		(stroke
			(width 0.25)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "56653110-5d89-4432-823d-7f2959615fdd")
	)
	(fp_line
		(start -2.05 -2.05)
		(end 2.05 -2.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "06592986-fc98-4adf-9535-03ff4ed7035f")
	)
	(fp_line
		(start -2.05 2.05)
		(end -2.05 -2.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "4ee3b01f-ad80-461e-ab46-aea3a65a9e3a")
	)
	(fp_line
		(start 2.05 -2.05)
		(end 2.05 2.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "29baf098-22ea-46c7-83de-361691f8c541")
	)
	(fp_line
		(start 2.05 2.05)
		(end -2.05 2.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "cccbbb15-139f-4ffd-a0c8-5700f65576dd")
	)
	(pad "1" smd roundrect
		(at -1.9846 -1.25)
		(size 0.96 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "69388b90-7ef3-459b-9d6b-a1c8d7f6774f")
	)
	(pad "2" smd roundrect
		(at -1.9846 -0.75)
		(size 0.96 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "bd3e57fe-13f0-4755-ac23-80587b95c06a")
	)
	(pad "3" smd roundrect
		(at -1.9846 -0.25)
		(size 0.96 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "49239330-9eea-4ac2-a20f-a27959733063")
	)
	(pad "4" smd roundrect
		(at -1.9846 0.25)
		(size 0.96 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "6f48f634-47d8-4722-91d2-0f7ed7c886b7")
	)
	(pad "5" smd roundrect
		(at -1.9846 0.75)
		(size 0.96 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "5f3140e2-7ee3-47b8-be2d-12757385e523")
	)
	(pad "6" smd roundrect
		(at -1.9846 1.25)
		(size 0.96 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "c5948c00-be66-440b-9930-2ab729b42d29")
	)
	(pad "7" smd roundrect
		(at -1.25 1.9846 90)
		(size 0.96 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "f9c55751-0dc3-43ef-93f5-79588ba769c1")
	)
	(pad "8" smd roundrect
		(at -0.75 1.9846 90)
		(size 0.96 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "77969189-5b78-496f-80b5-91dcabd836f8")
	)
	(pad "9" smd roundrect
		(at -0.25 1.9846 90)
		(size 0.96 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "2a2d7328-9110-4e41-8eb5-d4009d7fac93")
	)
	(pad "10" smd roundrect
		(at 0.25 1.9846 90)
		(size 0.96 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "c2a169a8-6f5c-4705-95f2-8d9043a09bbf")
	)
	(pad "11" smd roundrect
		(at 0.75 1.9846 90)
		(size 0.96 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "6a95f7ba-8725-4dce-8f62-1bef63f64ef4")
	)
	(pad "12" smd roundrect
		(at 1.25 1.9846 90)
		(size 0.96 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "64149f44-720c-4769-a168-c0d4264f979e")
	)
	(pad "13" smd roundrect
		(at 1.9846 1.25)
		(size 0.96 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "36b44d93-39da-4be9-a375-aca625221d39")
	)
	(pad "14" smd roundrect
		(at 1.9846 0.75)
		(size 0.96 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "98ab350e-9709-4a6e-9e4a-12930b515932")
	)
	(pad "15" smd roundrect
		(at 1.9846 0.25)
		(size 0.96 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "beada86f-daf8-46ef-9ee4-70971972abcb")
	)
	(pad "16" smd roundrect
		(at 1.9846 -0.25)
		(size 0.96 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "c9f067e4-b921-4610-a223-f60a0e38d681")
	)
	(pad "17" smd roundrect
		(at 1.9846 -0.75)
		(size 0.96 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "843fdf74-c970-4c2e-9c93-966fbd9a77a2")
	)
	(pad "18" smd roundrect
		(at 1.9846 -1.25)
		(size 0.96 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "6a163e9e-1294-4ed6-b81d-aff777331a63")
	)
	(pad "19" smd roundrect
		(at 1.25 -1.9846 90)
		(size 0.96 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "1bc18a81-bbee-4501-b940-316ecce4b1f5")
	)
	(pad "20" smd roundrect
		(at 0.75 -1.9846 90)
		(size 0.96 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "832d7d62-65fb-499e-81de-43caba9cbb7b")
	)
	(pad "21" smd roundrect
		(at 0.25 -1.9846 90)
		(size 0.96 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "98dcafb5-b99b-44e2-8ad2-beaa7893879c")
	)
	(pad "22" smd roundrect
		(at -0.25 -1.9846 90)
		(size 0.96 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "8cbce9ac-8381-4471-b2f9-e4089f10c9cd")
	)
	(pad "23" smd roundrect
		(at -0.75 -1.9846 90)
		(size 0.96 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "bc8c1e0b-ce7c-45c5-ad4b-3e958bbd7ff4")
	)
	(pad "24" smd roundrect
		(at -1.25 -1.9846 90)
		(size 0.96 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "e498a29f-5c16-478a-aaf2-08547f237594")
	)
	(pad "25" smd rect
		(at 0 0)
		(size 2.7 2.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(zone_connect 2)
		(thermal_bridge_angle 0)
		(uuid "2382b07b-6184-4091-8745-6f5b01c49a20")
	)
)