(footprint "SOP50P490X110-10N"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "10-SOP, 0.50 mm pitch, 4.90 mm span, 3.00 X 3.00 X 1.10 mm body\n\n10-pin SOP package with 0.50 mm pitch, 4.90 mm span with body size 3.00 X 3.00 X 1.10 mm")
	(property "Reference" "REF**"
		(at 0 -2.529 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "713e61c4-2163-4728-9ba3-cb445191525a")
		(effects
			(font
				(size 1.1684 1.1684)
				(thickness 0.1016)
			)
			(justify bottom)
		)
	)
	(property "Value" "SOP50P490X110-10N"
		(at 0 2.185 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "3a7e4c8d-7538-43e6-95cf-db6fd7ae1b4b")
		(effects
			(font
				(size 1.1684 1.1684)
				(thickness 0.1016)
			)
			(justify top)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "72864275-bf7c-40fb-8017-794a6c7e5484")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "f34ab9ac-1ae0-4e7c-a8c9-c251a994f59d")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "0de28211-73e6-459d-b487-098d78020564")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(fp_line
		(start -1.55 -1.55)
		(end 1.55 -1.55)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "949676a1-2def-4645-ba2c-1a28db43ce84")
	)
	(fp_line
		(start -1.55 -1.394)
		(end -1.55 -1.55)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "d3fb2feb-bb99-41c3-96da-5067766ea037")
	)
	(fp_line
		(start -1.55 1.394)
		(end -1.55 1.55)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "b724329a-5cfd-4236-a00c-899f206a3951")
	)
	(fp_line
		(start -1.55 1.55)
		(end 1.55 1.55)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "5b56f449-f9f2-47d4-a7f3-ce8ba541d245")
	)
	(fp_line
		(start 1.55 -1.55)
		(end 1.55 -1.394)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "3f9e448e-6b04-4b38-b1a2-f02b0980efca")
	)
	(fp_line
		(start 1.55 1.55)
		(end 1.55 1.394)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "7569f16a-aea0-4db7-bb5d-47b9abf0465c")
	)
	(fp_circle
		(center -2.2175 -1.644)
		(end -2.0925 -1.644)
		(stroke
			(width 0.25)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "336d8639-1993-40d5-9c09-71d1d1380c1b")
	)
	(fp_line
		(start -1.55 -1.55)
		(end 1.55 -1.55)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "fc55ea2b-4230-47a4-b9e5-b1a1295c20f1")
	)
	(fp_line
		(start -1.55 1.55)
		(end -1.55 -1.55)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "d8225673-8acd-4c2a-aa21-6756333d983e")
	)
	(fp_line
		(start 1.55 -1.55)
		(end 1.55 1.55)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f2e53e81-9834-4369-8028-d4874c6c3c54")
	)
	(fp_line
		(start 1.55 1.55)
		(end -1.55 1.55)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "a0a03cd4-a6b5-46cf-b875-089134113182")
	)
	(pad "1" smd roundrect
		(at -2.1496 -1)
		(size 1.4709 0.28)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "10e2a4fa-997c-4eb9-8db8-e3dea00ec163")
	)
	(pad "2" smd roundrect
		(at -2.1496 -0.5)
		(size 1.4709 0.28)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "b5d88990-7d13-41da-80fb-b1e57958be93")
	)
	(pad "3" smd roundrect
		(at -2.1496 0)
		(size 1.4709 0.28)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "dd348f59-75db-48a8-a159-3cbc1bbee0b7")
	)
	(pad "4" smd roundrect
		(at -2.1496 0.5)
		(size 1.4709 0.28)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "f3d95337-03de-4eaa-9449-c91fd240e92c")
	)
	(pad "5" smd roundrect
		(at -2.1496 1)
		(size 1.4709 0.28)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "9b30f570-c341-463f-9e8c-cf0c21f93b0b")
	)
	(pad "6" smd roundrect
		(at 2.1496 1)
		(size 1.4709 0.28)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "c4e8b76b-4927-48da-bdd0-c4cbffe09272")
	)
	(pad "7" smd roundrect
		(at 2.1496 0.5)
		(size 1.4709 0.28)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "330af068-745f-4ac2-9686-e41fd454a2c4")
	)
	(pad "8" smd roundrect
		(at 2.1496 0)
		(size 1.4709 0.28)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "74424c95-d323-4e9b-ad84-39917103d8db")
	)
	(pad "9" smd roundrect
		(at 2.1496 -0.5)
		(size 1.4709 0.28)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "cd5c54b7-543a-45d6-b607-13417f748899")
	)
	(pad "10" smd roundrect
		(at 2.1496 -1)
		(size 1.4709 0.28)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "d93a1752-dd30-43d8-a490-cea0dea32b28")
	)
)