(footprint "QFN50P700X700X60-49T560N"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "48-QFN, 0.50 mm pitch, 7.00 X 7.00 X 0.60 mm body, 5.60 X 5.60 mm thermal pad\n\n48-pin QFN package with 0.50 mm pitch with body size 7.00 X 7.00 X 0.60 mm and thermal pad size 5.60 X 5.60 mm")
	(property "Reference" "REF**"
		(at 0 -4.4996 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "26c78110-287e-47a8-9487-61d2536e52dd")
		(effects
			(font
				(size 1.1684 1.1684)
				(thickness 0.1016)
			)
			(justify bottom)
		)
	)
	(property "Value" "QFN50P700X700X60-49T560N"
		(at 0 4.4996 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "f6af12e9-73ee-47a1-9817-dc3a4a2c67c5")
		(effects
			(font
				(size 1.1684 1.1684)
				(thickness 0.1016)
			)
			(justify top)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "a2fc6f03-a87b-40e7-9cd0-5ef992c22e3c")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "a0a088f1-d24a-4862-89d3-d06aeaff0549")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "53f23bfa-dfaf-46d1-b1f9-a61424fe76fb")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(fp_line
		(start -3.55 -3.55)
		(end -3.139 -3.55)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "5717c763-b696-49cd-a52b-886bbd6d1e33")
	)
	(fp_line
		(start -3.55 -3.139)
		(end -3.55 -3.55)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2428625d-b5fc-4a8d-9def-e4dd20c06ef9")
	)
	(fp_line
		(start -3.55 3.139)
		(end -3.55 3.55)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "4d6baeae-1d22-409d-871d-379459133a66")
	)
	(fp_line
		(start -3.55 3.55)
		(end -3.139 3.55)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "040750ef-6580-4390-9f65-2a493eb6de59")
	)
	(fp_line
		(start 3.55 -3.55)
		(end 3.139 -3.55)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "1c6dbfe3-9616-485b-a301-efbb25a33641")
	)
	(fp_line
		(start 3.55 -3.139)
		(end 3.55 -3.55)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "336019ce-7d98-412d-8917-bd01834381bf")
	)
	(fp_line
		(start 3.55 3.139)
		(end 3.55 3.55)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "15bd1342-4c50-49cb-8958-d691ad45f0c3")
	)
	(fp_line
		(start 3.55 3.55)
		(end 3.139 3.55)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "5402abf8-e1e3-487a-b873-d3b6345a3519")
	)
	(fp_circle
		(center -4.054 -3.389)
		(end -3.929 -3.389)
		(stroke
			(width 0.25)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "bdf6d605-7c33-43d8-82f0-7b91e380e029")
	)
	(fp_line
		(start -3.55 -3.55)
		(end 3.55 -3.55)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c6b78178-d583-4e5f-be05-fda6cf90f87f")
	)
	(fp_line
		(start -3.55 3.55)
		(end -3.55 -3.55)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "15c46425-e4cc-43bf-866e-c9c3eea73063")
	)
	(fp_line
		(start 3.55 -3.55)
		(end 3.55 3.55)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "a8d73170-a459-438d-9ae4-a9f764fd51f4")
	)
	(fp_line
		(start 3.55 3.55)
		(end -3.55 3.55)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "3dbe4cae-da0a-4793-8adb-2d4eb59c148f")
	)
	(pad "1" smd roundrect
		(at -3.4346 -2.75)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "21a50ab0-8c2b-4bc4-894f-d67ba6a9067e")
	)
	(pad "2" smd roundrect
		(at -3.4346 -2.25)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "bdeb6b7e-1abd-40c3-ab88-ff47ac9ef761")
	)
	(pad "3" smd roundrect
		(at -3.4346 -1.75)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "a7acc791-eb74-4a01-a914-7fbec3d56590")
	)
	(pad "4" smd roundrect
		(at -3.4346 -1.25)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "afb845d7-f641-4298-baed-6cf48473723f")
	)
	(pad "5" smd roundrect
		(at -3.4346 -0.75)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "b826bfd2-1ea9-4bcf-a56d-7b19712f8521")
	)
	(pad "6" smd roundrect
		(at -3.4346 -0.25)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "07c85b97-bef7-4b0d-b3b9-2bdfc533ec9f")
	)
	(pad "7" smd roundrect
		(at -3.4346 0.25)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "66d7bd1c-311e-4d0a-b9f9-9ce7fd2fdf89")
	)
	(pad "8" smd roundrect
		(at -3.4346 0.75)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "387ed576-859b-44fe-b3a4-bb97a77baa20")
	)
	(pad "9" smd roundrect
		(at -3.4346 1.25)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "a78685aa-5d93-40f0-9f96-26e600ab6e16")
	)
	(pad "10" smd roundrect
		(at -3.4346 1.75)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "95ffbbe2-74c9-4c07-b0a8-9384922c23eb")
	)
	(pad "11" smd roundrect
		(at -3.4346 2.25)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "86ec01b5-588d-4b7e-a5c5-38853b6a070f")
	)
	(pad "12" smd roundrect
		(at -3.4346 2.75)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "5e53d956-16e1-43e2-80d8-ccb045764402")
	)
	(pad "13" smd roundrect
		(at -2.75 3.4346 90)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "98f30132-361e-4443-baeb-8f7b6a0da2e0")
	)
	(pad "14" smd roundrect
		(at -2.25 3.4346 90)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "69224f2d-76df-49b9-a9d7-debb465af32e")
	)
	(pad "15" smd roundrect
		(at -1.75 3.4346 90)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "1f2d995f-5431-483a-88eb-3274bff80f10")
	)
	(pad "16" smd roundrect
		(at -1.25 3.4346 90)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "514f1cc2-7ea0-4e57-8644-cd9b75d0895c")
	)
	(pad "17" smd roundrect
		(at -0.75 3.4346 90)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "b87f3eba-8bdd-415d-8af5-fc191c5836d4")
	)
	(pad "18" smd roundrect
		(at -0.25 3.4346 90)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "01830cca-0504-4931-8e8c-959183022077")
	)
	(pad "19" smd roundrect
		(at 0.25 3.4346 90)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "c38dfb4b-8afc-48c3-ba73-c2d78bbcde4a")
	)
	(pad "20" smd roundrect
		(at 0.75 3.4346 90)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "6e562708-0821-4ad3-ba93-8c596639caeb")
	)
	(pad "21" smd roundrect
		(at 1.25 3.4346 90)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "388141e0-6201-4259-be71-17982fd3e126")
	)
	(pad "22" smd roundrect
		(at 1.75 3.4346 90)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "605bd06c-dbb0-47eb-b3cf-8662b6136fdc")
	)
	(pad "23" smd roundrect
		(at 2.25 3.4346 90)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "718f785f-c4f5-428c-9b37-c4d4d355d802")
	)
	(pad "24" smd roundrect
		(at 2.75 3.4346 90)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "5adc9d7c-5a9a-4d95-b84c-4a28c07687af")
	)
	(pad "25" smd roundrect
		(at 3.4346 2.75)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "81292dec-15b4-439e-bddf-3ff5e66926a5")
	)
	(pad "26" smd roundrect
		(at 3.4346 2.25)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "890a5a62-c1e2-49bc-8896-e1ffbc325a10")
	)
	(pad "27" smd roundrect
		(at 3.4346 1.75)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "1c58bc0e-94d1-4bc3-9800-14349cdb566d")
	)
	(pad "28" smd roundrect
		(at 3.4346 1.25)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "af0c0f98-8827-44e3-adfc-9b2a6315a599")
	)
	(pad "29" smd roundrect
		(at 3.4346 0.75)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "8b0b562b-f7fa-4d8e-aa2a-16f18503c62e")
	)
	(pad "30" smd roundrect
		(at 3.4346 0.25)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "c08f9e91-d169-4a67-819c-58eb1c1de358")
	)
	(pad "31" smd roundrect
		(at 3.4346 -0.25)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "59505fa1-dfab-49a6-930e-315cfebfd59d")
	)
	(pad "32" smd roundrect
		(at 3.4346 -0.75)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "2402183d-8afe-4076-8deb-94879f5e8e37")
	)
	(pad "33" smd roundrect
		(at 3.4346 -1.25)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "68c26258-349b-4f05-883c-192324963985")
	)
	(pad "34" smd roundrect
		(at 3.4346 -1.75)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "90cb40d8-4af5-478b-b262-4b104e626aae")
	)
	(pad "35" smd roundrect
		(at 3.4346 -2.25)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "aa67b568-e2c6-4347-969f-024121d19094")
	)
	(pad "36" smd roundrect
		(at 3.4346 -2.75)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "fc9d2226-db70-4f36-8e4e-39e245941a96")
	)
	(pad "37" smd roundrect
		(at 2.75 -3.4346 90)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "6f4bf433-9367-4432-9afe-03647c1749ec")
	)
	(pad "38" smd roundrect
		(at 2.25 -3.4346 90)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "a9c25187-7b2e-4e8b-afa7-55f51368df26")
	)
	(pad "39" smd roundrect
		(at 1.75 -3.4346 90)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "68ce2765-bf41-45aa-bd67-993ed3bab08b")
	)
	(pad "40" smd roundrect
		(at 1.25 -3.4346 90)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "c6541bd0-58c0-4487-a00d-bd2ec30e9ded")
	)
	(pad "41" smd roundrect
		(at 0.75 -3.4346 90)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "de0cb8f8-419b-46a2-a335-5d79297bfc7a")
	)
	(pad "42" smd roundrect
		(at 0.25 -3.4346 90)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "b1de5e65-8e57-456d-8ddb-bff0ed7f62f4")
	)
	(pad "43" smd roundrect
		(at -0.25 -3.4346 90)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "37476eea-5157-4b2f-b564-d4ab9a84b0f6")
	)
	(pad "44" smd roundrect
		(at -0.75 -3.4346 90)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "063b7835-4ccc-45a8-879b-31189665999f")
	)
	(pad "45" smd roundrect
		(at -1.25 -3.4346 90)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "40e8d62a-81df-4226-9296-808ea19ba78f")
	)
	(pad "46" smd roundrect
		(at -1.75 -3.4346 90)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "4049d12a-712f-47b3-90ec-f3656a84b4dc")
	)
	(pad "47" smd roundrect
		(at -2.25 -3.4346 90)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "6f7beaf8-2339-4fe1-a74a-5b652352acac")
	)
	(pad "48" smd roundrect
		(at -2.75 -3.4346 90)
		(size 0.86 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.5)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "48462497-4816-4f16-a7aa-be046fea84f0")
	)
	(pad "49" smd rect
		(at 0 0)
		(size 5.6 5.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(zone_connect 2)
		(thermal_bridge_angle 0)
		(uuid "281b9f7e-b3fe-4a4e-a172-05efd48b508d")
	)
)