(footprint "TYPE-C16P"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "3b988ee5-04d3-4690-a0f5-2e3be8484744")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Value" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "e5fd0aef-f18e-409e-ab57-89e4f90b6feb")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "7551f33d-91e8-45c5-bb2f-3645ff9e5d72")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "5d8e7f1d-da99-46b2-a99b-ffb5e1516768")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "e9c133e3-4457-4ebb-bc7f-5317a8136382")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(fp_line
		(start -4.5 0.3)
		(end 4.5 0.3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "ff668aff-b9b0-4b67-b551-cc3a65d9bc46")
	)
	(fp_line
		(start -4.5 7.9)
		(end -4.5 0.3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "e80302c5-b63d-4f47-8eae-0174b46c366d")
	)
	(fp_line
		(start 4.5 0.3)
		(end 4.5 7.9)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "81367532-2e60-4ca3-8894-1037a7a8988d")
	)
	(fp_line
		(start 4.5 7.9)
		(end -4.5 7.9)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "a8cfa656-407f-4f83-baf4-d6908964e20b")
	)
	(pad "" np_thru_hole circle
		(at -2.89 1.6)
		(size 0.6 0.6)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(uuid "38154fd2-a772-4560-816d-221c98c214d7")
	)
	(pad "" np_thru_hole circle
		(at 2.89 1.6)
		(size 0.6 0.6)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(uuid "7536beea-5b27-408c-9de3-9cdf68d4d1d7")
	)
	(pad "1" smd rect
		(at -3.2 0.5 90)
		(size 1 0.52)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "55a01b44-9aab-4ca2-966e-133ab24599e6")
	)
	(pad "2" smd rect
		(at -2.4 0.5 90)
		(size 1 0.52)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "e48951d8-92e7-4c3e-8bc6-8af11bce5131")
	)
	(pad "3" smd rect
		(at -1.75 0.5 270)
		(size 1 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "9d44c46c-3836-4912-b368-b0c1055066dc")
	)
	(pad "4" smd rect
		(at -1.25 0.5 270)
		(size 1 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "e8fd70a3-3ebf-4d03-8050-ac5e996f598b")
	)
	(pad "5" smd rect
		(at -0.75 0.5 270)
		(size 1 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "9fb15b09-dd74-4a76-a271-926718cd2022")
	)
	(pad "6" smd rect
		(at -0.25 0.5 270)
		(size 1 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "bfaf4506-dba5-49e2-b16d-491f963afbf9")
	)
	(pad "7" smd rect
		(at 0.25 0.5 270)
		(size 1 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "549d760a-aceb-4be4-9f01-e27f39a4973d")
	)
	(pad "8" smd rect
		(at 0.75 0.5 270)
		(size 1 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "cca8a762-0a73-4c66-b31d-de16b8633585")
	)
	(pad "9" smd rect
		(at 1.25 0.5 270)
		(size 1 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "857eec99-be96-4fc9-8317-ebaf95e328d5")
	)
	(pad "10" smd rect
		(at 1.75 0.5 270)
		(size 1 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "98aec5ed-8d10-4ba4-8588-c19dc360a84e")
	)
	(pad "11" smd rect
		(at 2.4 0.5 90)
		(size 1 0.52)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "5370007e-6f09-42e3-88da-e1159086b056")
	)
	(pad "12" smd rect
		(at 3.2 0.5 90)
		(size 1 0.52)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "b4fed87b-a0e2-4098-ad39-5971323d0f56")
	)
	(pad "M1" thru_hole oval
		(at -4.3 5.3 90)
		(size 2.2 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "94c020cd-45d4-4a6b-bd78-03793e5bc54c")
	)
	(pad "M2" thru_hole oval
		(at -4.32 1.1 90)
		(size 2.2 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "ce76bc57-58ad-40d9-a61b-a717d2321466")
	)
	(pad "M3" thru_hole oval
		(at 4.32 5.3 90)
		(size 2.2 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "cedd4603-d2e1-4241-8213-baf4bdd81f65")
	)
	(pad "M4" thru_hole oval
		(at 4.32 1.1 90)
		(size 2.2 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "e5e6dab7-6bb1-4e8a-8098-d5926afa9b52")
	)
)