<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.1">
<drawing>
<library>
<description>Generated from &lt;b&gt;VNA.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="NFM15PC">
</package>
<package name="MSOP8">
</package>
<package name="SON50P400X500X80-17T260X400N">
<description>16-SON (DFN), 0.50 mm pitch, 5.00 X 4.00 X 0.80 mm body, 4.00 X 2.60 mm thermal pad
&lt;p&gt;16-pin SON (DFN) package with 0.50 mm pitch with body size 5.00 X 4.00 X 0.80 mm and thermal pad size 4.00 X 2.60 mm&lt;/p&gt;</description>
</package>
<package name="QFN50P400X400X75-21T206">
<description>20-QFN, 0.50 mm pitch, 4.00 X 4.00 X 0.75 mm body, 2.06 X 2.06 mm thermal pad
&lt;p&gt;20-pin QFN package with 0.50 mm pitch with body size 4.00 X 4.00 X 0.75 mm and thermal pad size 2.06 X 2.06 mm&lt;/p&gt;</description>
</package>
<package name="QFN50P400X400X90-21T270N">
<description>20-QFN, 0.50 mm pitch, 4.00 X 4.00 X 0.90 mm body, 2.70 X 2.70 mm thermal pad
&lt;p&gt;20-pin QFN package with 0.50 mm pitch with body size 4.00 X 4.00 X 0.90 mm and thermal pad size 2.70 X 2.70 mm&lt;/p&gt;</description>
</package>
<package name="SO08">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
150 mil (3.9 mm) body/JEDEC MS-012AA</description>
</package>
<package name="J502-ND-142-0711-821/826">
<description>&lt;b&gt;SMA 50 Ohm&lt;/b&gt; Board Thickness &lt;b&gt;0.062&lt;/b&gt; Inch, End Launch Jack Receptacle&lt;p&gt;
Johnson Components&lt;br&gt;
Source: www.johnsoncomponents.com .. J502-ND.pdf</description>
</package>
<package name="SOP50P490X110-10N">
<description>10-SOP, 0.50 mm pitch, 4.90 mm span, 3.00 X 3.00 X 1.10 mm body
&lt;p&gt;10-pin SOP package with 0.50 mm pitch, 4.90 mm span with body size 3.00 X 3.00 X 1.10 mm&lt;/p&gt;</description>
</package>
<package name="INDC2012X100N">
<description>Chip, 2.00 X 1.25 X 1.00 mm body
&lt;p&gt;Chip package with body size 2.00 X 1.25 X 1.00 mm&lt;/p&gt;</description>
</package>
<package name="QFN50P500X500X80-33T310">
<description>32-QFN, 0.50 mm pitch, 5.00 X 5.00 X 0.80 mm body, 3.10 X 3.10 mm thermal pad
&lt;p&gt;32-pin QFN package with 0.50 mm pitch with body size 5.00 X 5.00 X 0.80 mm and thermal pad size 3.10 X 3.10 mm&lt;/p&gt;</description>
</package>
<package name="SRN5040">
</package>
<package name="FA-128">
<description>&lt;b&gt;&lt;b&gt;MHZ RANGE CRYSTASL UNIT&lt;/b&gt;&lt;/b&gt; FA-128&lt;p&gt;
ULTRA MINIATURE SIZE LOW PROFILE SMD&lt;br&gt;
Source: Epson Toyocom FA128.pdf</description>
</package>
<package name="SOT95P240X110-5">
<description>5-SOT23, 0.95 mm pitch, 2.40 mm span, 2.90 X 1.30 X 1.10 mm body
&lt;p&gt;5-pin SOT23 package with 0.95 mm pitch, 2.40 mm span with body size 2.90 X 1.30 X 1.10 mm&lt;/p&gt;</description>
</package>
<package name="L0402">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R0402">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="SON50P200X200X80-9T90X160N">
<description>8-SON (DFN), 0.50 mm pitch, 2.00 X 2.00 X 0.80 mm body, 1.60 X 0.90 mm thermal pad
&lt;p&gt;8-pin SON (DFN) package with 0.50 mm pitch with body size 2.00 X 2.00 X 0.80 mm and thermal pad size 1.60 X 0.90 mm&lt;/p&gt;</description>
</package>
<package name="B1,27">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="CHIPLED_0603">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY Q971.pdf</description>
</package>
<package name="DCJ0202">
<description>&lt;b&gt;DC POWER JACK&lt;/b&gt;&lt;p&gt;
Source: DCJ0202.pdf</description>
</package>
<package name="SMB">
<description>&lt;b&gt;DIODE&lt;/b&gt;</description>
</package>
<package name="QFN50P500X500X100-33T345N">
<description>32-QFN, 0.50 mm pitch, 5.00 X 5.00 X 1.00 mm body, 3.45 X 3.45 mm thermal pad
&lt;p&gt;32-pin QFN package with 0.50 mm pitch with body size 5.00 X 5.00 X 1.00 mm and thermal pad size 3.45 X 3.45 mm&lt;/p&gt;</description>
</package>
<package name="SOT230P700X180-4">
<description>4-SOT223, 2.30 mm pitch, 7.00 mm span, 6.50 X 3.50 X 1.80 mm body
&lt;p&gt;4-pin SOT223 package with 2.30 mm pitch, 7.00 mm span with body size 6.50 X 3.50 X 1.80 mm&lt;/p&gt;</description>
</package>
<package name="C0402">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="AMPHENOL_132289">
</package>
<package name="1X10/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="NFM18PC">
</package>
<package name="NFM21PC">
</package>
<package name="TQ144">
<description>&lt;b&gt;TQ144 TQG144&lt;/b&gt;</description>
</package>
<package name="SON50P300X300X90-13T170X240N">
<description>12-SON (DFN), 0.50 mm pitch, 3.00 X 3.00 X 0.90 mm body, 2.40 X 1.70 mm thermal pad
&lt;p&gt;12-pin SON (DFN) package with 0.50 mm pitch with body size 3.00 X 3.00 X 0.90 mm and thermal pad size 2.40 X 1.70 mm&lt;/p&gt;</description>
</package>
<package name="SOP65P490X110-8N">
<description>8-SOP, 0.65 mm pitch, 4.90 mm span, 3.00 X 3.00 X 1.10 mm body
&lt;p&gt;8-pin SOP package with 0.65 mm pitch, 4.90 mm span with body size 3.00 X 3.00 X 1.10 mm&lt;/p&gt;</description>
</package>
<package name="EASTEVER_BALUN">
</package>
<package name="SON95P300X300X100-7T170X240N">
<description>6-SON (DFN), 0.95 mm pitch, 3.00 X 3.00 X 1.00 mm body, 2.40 X 1.70 mm thermal pad
&lt;p&gt;6-pin SON (DFN) package with 0.95 mm pitch with body size 3.00 X 3.00 X 1.00 mm and thermal pad size 2.40 X 1.70 mm&lt;/p&gt;</description>
</package>
<package name="QFN40P180X180X55-13T76N">
<description>12-QFN, 0.40 mm pitch, 1.80 X 1.80 X 0.55 mm body, 0.76 X 0.76 mm thermal pad
&lt;p&gt;12-pin QFN package with 0.40 mm pitch with body size 1.80 X 1.80 X 0.55 mm and thermal pad size 0.76 X 0.76 mm&lt;/p&gt;</description>
</package>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="TYPE-C16P">
</package>
<package name="QFN50P700X700X60-49T560N">
<description>48-QFN, 0.50 mm pitch, 7.00 X 7.00 X 0.60 mm body, 5.60 X 5.60 mm thermal pad
&lt;p&gt;48-pin QFN package with 0.50 mm pitch with body size 7.00 X 7.00 X 0.60 mm and thermal pad size 5.60 X 5.60 mm&lt;/p&gt;</description>
</package>
<package name="32005-301">
<description>&lt;b&gt;MINI USB-B R/A SMT W/O REAR&lt;/b&gt;&lt;p&gt;
Source: http://www.cypressindustries.com/pdf/32005-301.pdf</description>
</package>
<package name="FILTRDFN160X84X70-4N">
<description>DFN4, 1.60 X 0.84 X 0.70 mm body
&lt;p&gt;DFN4 package with body size 1.60 X 0.84 X 0.70 mm&lt;/p&gt;</description>
</package>
<package name="QFN50P600X600X100-37T410N">
<description>36-QFN, 0.50 mm pitch, 6.00 X 6.00 X 1.00 mm body, 4.10 X 4.10 mm thermal pad
&lt;p&gt;36-pin QFN package with 0.50 mm pitch with body size 6.00 X 6.00 X 1.00 mm and thermal pad size 4.10 X 4.10 mm&lt;/p&gt;</description>
</package>
<package name="PJ-014D">
</package>
<package name="QFN50P400X400X75-25T270">
<description>24-QFN, 0.50 mm pitch, 4.00 X 4.00 X 0.75 mm body, 2.70 X 2.70 mm thermal pad
&lt;p&gt;24-pin QFN package with 0.50 mm pitch with body size 4.00 X 4.00 X 0.75 mm and thermal pad size 2.70 X 2.70 mm&lt;/p&gt;</description>
</package>
<package name="SOTFL95P240X80-3N">
<description>3-SOTFL, 0.95 mm pitch, 2.40 mm span, 2.90 X 1.80 X 0.80 mm body
&lt;p&gt;3-pin SOTFL package with 0.95 mm pitch, 2.40 mm span with body size 2.90 X 1.80 X 0.80 mm&lt;/p&gt;</description>
</package>
<package name="QFN50P400X400X100-25T250N">
<description>24-QFN, 0.50 mm pitch, 4.00 X 4.00 X 1.00 mm body, 2.50 X 2.50 mm thermal pad
&lt;p&gt;24-pin QFN package with 0.50 mm pitch with body size 4.00 X 4.00 X 1.00 mm and thermal pad size 2.50 X 2.50 mm&lt;/p&gt;</description>
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="SON50P300X300X80-9T165X238">
<description>8-SON, 0.50 mm pitch, 3.00 X 3.00 X 0.80 mm body, 2.38 X 1.65 mm thermal pad
&lt;p&gt;8-pin SON package with 0.50 mm pitch with body size 3.00 X 3.00 X 0.80 mm and thermal pad size 2.38 X 1.65 mm&lt;/p&gt;</description>
</package>
<package name="2X10">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="TE_2118718-2">
</package>
<package name="AMPHENOL_901-10510-2">
</package>
<package name="BU-1420701851">
</package>
<package name="PAT0816">
</package>
</packages>
<symbols>
<symbol name="BNC-FGND">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="LM3370_BUCK">
<pin name="VIN"/>
<pin name="SW"/>
<pin name="PGND"/>
<pin name="FB"/>
<pin name="EN"/>
<pin name="/POR"/>
</symbol>
<symbol name="GND">
<pin name="GND" direction="sup"/>
</symbol>
<symbol name="QPC6324">
<pin name="CTL1"/>
<pin name="CTL2"/>
<pin name="GND"/>
<pin name="RF1"/>
<pin name="RF2"/>
<pin name="RF_COM"/>
<pin name="VCC"/>
</symbol>
<symbol name="LM3370_CONTROL">
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="VDD"/>
<pin name="SGND"/>
</symbol>
<symbol name="25XX">
<pin name="!CS!" direction="in"/>
<pin name="!HOLD!" direction="in"/>
<pin name="!WP!" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="DI" direction="in"/>
<pin name="DO" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="SI5351C">
<pin name="CLK0"/>
<pin name="CLK1"/>
<pin name="CLK2"/>
<pin name="CLK3"/>
<pin name="CLK4"/>
<pin name="CLK5"/>
<pin name="CLK6"/>
<pin name="CLK7"/>
<pin name="CLKIN"/>
<pin name="GND"/>
<pin name="INTR"/>
<pin name="OEB"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="VDD"/>
<pin name="VDDOA"/>
<pin name="VDDOB"/>
<pin name="VDDOC"/>
<pin name="VDDOD"/>
<pin name="XA"/>
<pin name="XB"/>
</symbol>
<symbol name="MCP33131D-10-E/MS">
<pin name="AIN+"/>
<pin name="AIN-"/>
<pin name="AVDD"/>
<pin name="CONVST"/>
<pin name="DVIO"/>
<pin name="GND"/>
<pin name="SCLK"/>
<pin name="SDI"/>
<pin name="SDO"/>
<pin name="VREF"/>
</symbol>
<symbol name="L-EU">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="VCCINT">
<pin name="VCCINT" direction="sup"/>
</symbol>
<symbol name="+05V/1">
<pin name="+5V/1" direction="sup"/>
</symbol>
<symbol name="VREG_EN">
<pin name="EN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="VOUT" direction="pwr"/>
</symbol>
<symbol name="MAX2871">
<pin name="BIAS_FILT"/>
<pin name="CE"/>
<pin name="CLK" direction="in"/>
<pin name="CP_OUT"/>
<pin name="DATA" direction="in"/>
<pin name="EP"/>
<pin name="GND_CP"/>
<pin name="GND_DIG"/>
<pin name="GND_PLL"/>
<pin name="GND_RF"/>
<pin name="GND_SD"/>
<pin name="GND_TUNE"/>
<pin name="GND_VCO"/>
<pin name="LD" direction="out"/>
<pin name="LE" direction="in"/>
<pin name="MUX"/>
<pin name="NOISE_FILT"/>
<pin name="REF_IN" direction="in"/>
<pin name="REG"/>
<pin name="RFOUTA_N"/>
<pin name="RFOUTA_P"/>
<pin name="RFOUTB_N"/>
<pin name="RFOUTB_P"/>
<pin name="RFOUT_EN" direction="in"/>
<pin name="RSET"/>
<pin name="SW"/>
<pin name="TUNE"/>
<pin name="VCC_CP"/>
<pin name="VCC_DIG"/>
<pin name="VCC_PLL"/>
<pin name="VCC_RF"/>
<pin name="VCC_VCO"/>
<pin name="VDD_SD"/>
</symbol>
<symbol name="Q-SHIELD2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="AMPLIFIER_PWDN">
<pin name="GND"/>
<pin name="PWDN"/>
<pin name="RFIN"/>
<pin name="RFOUT"/>
<pin name="VCC"/>
</symbol>
<symbol name="+05V/2">
<pin name="+5V/2" direction="sup"/>
</symbol>
<symbol name="L-EU:1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="R-EU">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="LED">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="A3L-LOC">
</symbol>
<symbol name="TP">
<pin name="TP" direction="in"/>
</symbol>
<symbol name="+3V3">
<pin name="+3V3" direction="sup"/>
</symbol>
<symbol name="DC-JACK-SWITCH">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="TPS65265COM">
<pin name="AGND"/>
<pin name="MODE"/>
<pin name="PGOOD"/>
<pin name="PG_DLY"/>
<pin name="PSM"/>
<pin name="ROSC"/>
<pin name="SEQ_DLY"/>
<pin name="V7V"/>
</symbol>
<symbol name="TPS65265BUCK">
<pin name="BST"/>
<pin name="COMP"/>
<pin name="EN"/>
<pin name="FB"/>
<pin name="GND"/>
<pin name="LX"/>
<pin name="VIN"/>
</symbol>
<symbol name="+12V">
<pin name="+12V" direction="sup"/>
</symbol>
<symbol name="D">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="VREG">
<pin name="GND" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="VOUT" direction="pwr"/>
</symbol>
<symbol name="C-EU:1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="COAX">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="6SLX9TQG144_1">
<pin name="IO_L1N_VREF_1"/>
<pin name="IO_L1P_1"/>
<pin name="IO_L32N_1"/>
<pin name="IO_L32P_1"/>
<pin name="IO_L33N_1"/>
<pin name="IO_L33P_1"/>
<pin name="IO_L34N_1"/>
<pin name="IO_L34P_1"/>
<pin name="IO_L40N_GCLK10_1"/>
<pin name="IO_L40P_GCLK11_1"/>
<pin name="IO_L41N_GCLK8_1"/>
<pin name="IO_L41P_GCLK9_IRDY1_1"/>
<pin name="IO_L42N_GCLK6_TRDY1_1"/>
<pin name="IO_L42P_GCLK7_1"/>
<pin name="IO_L43N_GCLK4_1"/>
<pin name="IO_L43P_GCLK5_1"/>
<pin name="IO_L45N_1"/>
<pin name="IO_L45P_1"/>
<pin name="IO_L46N_1"/>
<pin name="IO_L46P_1"/>
<pin name="IO_L47N_1"/>
<pin name="IO_L47P_1"/>
<pin name="IO_L74N_DOUT_BUSY_1"/>
<pin name="IO_L74P_AWAKE_1"/>
<pin name="VCCO_1@0" direction="in"/>
<pin name="VCCO_1@1" direction="in"/>
<pin name="VCCO_1@2" direction="in"/>
</symbol>
<symbol name="6SLX9TQG144_2">
<pin name="CMPCS_B_2"/>
<pin name="DONE_2"/>
<pin name="IO_L1N_M0_CMPMISO_2"/>
<pin name="IO_L1P_CCLK_2"/>
<pin name="IO_L2N_CMPMOSI_2"/>
<pin name="IO_L2P_CMPCLK_2"/>
<pin name="IO_L3N_MOSI_CSI_B_MISO0_2"/>
<pin name="IO_L3P_D0_DIN_MISO_MISO1_2"/>
<pin name="IO_L12N_D2_MISO3_2"/>
<pin name="IO_L12P_D1_MISO2_2"/>
<pin name="IO_L13N_D10_2"/>
<pin name="IO_L13P_M1_2"/>
<pin name="IO_L14N_D12_2"/>
<pin name="IO_L14P_D11_2"/>
<pin name="IO_L30N_GCLK0_USERCCLK_2"/>
<pin name="IO_L30P_GCLK1_D13_2"/>
<pin name="IO_L31N_GCLK30_D15_2"/>
<pin name="IO_L31P_GCLK31_D14_2"/>
<pin name="IO_L48N_RDWR_B_VREF_2"/>
<pin name="IO_L48P_D7_2"/>
<pin name="IO_L49N_D4_2"/>
<pin name="IO_L49P_D3_2"/>
<pin name="IO_L62N_D6_2"/>
<pin name="IO_L62P_D5_2"/>
<pin name="IO_L64N_D9_2"/>
<pin name="IO_L64P_D8_2"/>
<pin name="IO_L65N_CSO_B_2"/>
<pin name="IO_L65P_INIT_B_2"/>
<pin name="PROGRAM_B_2" direction="in"/>
<pin name="VCCO_2@0" direction="in"/>
<pin name="VCCO_2@1" direction="in"/>
</symbol>
<symbol name="6SLX9TQG144_3">
<pin name="IO_L1N_VREF_3"/>
<pin name="IO_L1P_3"/>
<pin name="IO_L2N_3"/>
<pin name="IO_L2P_3"/>
<pin name="IO_L36N_3"/>
<pin name="IO_L36P_3"/>
<pin name="IO_L37N_3"/>
<pin name="IO_L37P_3"/>
<pin name="IO_L41N_GCLK26_3"/>
<pin name="IO_L41P_GCLK27_3"/>
<pin name="IO_L42N_GCLK24_3"/>
<pin name="IO_L42P_GCLK25_TRDY2_3"/>
<pin name="IO_L43N_GCLK22_IRDY2_3"/>
<pin name="IO_L43P_GCLK23_3"/>
<pin name="IO_L44N_GCLK20_3"/>
<pin name="IO_L44P_GCLK21_3"/>
<pin name="IO_L49N_3"/>
<pin name="IO_L49P_3"/>
<pin name="IO_L50N_3"/>
<pin name="IO_L50P_3"/>
<pin name="IO_L51N_3"/>
<pin name="IO_L51P_3"/>
<pin name="IO_L52N_3"/>
<pin name="IO_L52P_3"/>
<pin name="IO_L83N_VREF_3"/>
<pin name="IO_L83P_3"/>
<pin name="VCCO_3@0" direction="in"/>
<pin name="VCCO_3@1" direction="in"/>
<pin name="VCCO_3@2" direction="in"/>
</symbol>
<symbol name="6SLX9TQG144_0">
<pin name="IO_L1N_VREF_0"/>
<pin name="IO_L1P_HSWAPEN_0"/>
<pin name="IO_L2N_0"/>
<pin name="IO_L2P_0"/>
<pin name="IO_L3N_0"/>
<pin name="IO_L3P_0"/>
<pin name="IO_L4N_0"/>
<pin name="IO_L4P_0"/>
<pin name="IO_L34N_GCLK18_0"/>
<pin name="IO_L34P_GCLK19_0"/>
<pin name="IO_L35N_GCLK16_0"/>
<pin name="IO_L35P_GCLK17_0"/>
<pin name="IO_L36N_GCLK14_0"/>
<pin name="IO_L36P_GCLK15_0"/>
<pin name="IO_L37N_GCLK12_0"/>
<pin name="IO_L37P_GCLK13_0"/>
<pin name="IO_L62N_VREF_0"/>
<pin name="IO_L62P_0"/>
<pin name="IO_L63N_SCP6_0"/>
<pin name="IO_L63P_SCP7_0"/>
<pin name="IO_L64N_SCP4_0"/>
<pin name="IO_L64P_SCP5_0"/>
<pin name="IO_L65N_SCP2_0"/>
<pin name="IO_L65P_SCP3_0"/>
<pin name="IO_L66N_SCP0_0"/>
<pin name="IO_L66P_SCP1_0"/>
<pin name="VCCO_0@0" direction="in"/>
<pin name="VCCO_0@1" direction="in"/>
<pin name="VCCO_0@2" direction="in"/>
</symbol>
<symbol name="6SLX9TQG144_VCCAUX">
<pin name="VCCAUX@0" direction="in"/>
<pin name="VCCAUX@1" direction="in"/>
<pin name="VCCAUX@2" direction="in"/>
<pin name="VCCAUX@3" direction="in"/>
<pin name="VCCAUX@4" direction="in"/>
</symbol>
<symbol name="6SLX9TQG144_NA">
<pin name="SUSPEND" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="TMS" direction="in"/>
</symbol>
<symbol name="PINHD10">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
</symbol>
<symbol name="6SLX9TQG144_GND">
<pin name="GND@0" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
<pin name="GND@9" direction="pwr"/>
<pin name="GND@10" direction="pwr"/>
<pin name="GND@11" direction="pwr"/>
<pin name="GND@12" direction="pwr"/>
</symbol>
<symbol name="6SLX9TQG144_VCCINT">
<pin name="VCCINT@0" direction="in"/>
<pin name="VCCINT@1" direction="in"/>
<pin name="VCCINT@2" direction="in"/>
<pin name="VCCINT@3" direction="in"/>
<pin name="VCCINT@4" direction="in"/>
</symbol>
<symbol name="LDL212">
<pin name="EN"/>
<pin name="GND"/>
<pin name="SENSE"/>
<pin name="VIN"/>
<pin name="VOUT"/>
</symbol>
<symbol name="C-FILTER">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="2@1" direction="pas"/>
<pin name="2@2" direction="pas"/>
</symbol>
<symbol name="MIC2253">
<pin name="AGND"/>
<pin name="PGND"/>
<pin name="COMP"/>
<pin name="SS"/>
<pin name="EN"/>
<pin name="VIN"/>
<pin name="SW"/>
<pin name="OVP"/>
<pin name="FB"/>
</symbol>
<symbol name="BALUN_1:1">
<pin name="IN+"/>
<pin name="IN-"/>
<pin name="OUT+"/>
<pin name="OUT-"/>
</symbol>
<symbol name="OPAMPDIFF_SHDN">
<pin name="+IN" direction="in"/>
<pin name="+OUT"/>
<pin name="-IN" direction="in"/>
<pin name="-OUT"/>
<pin name="SHDN"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="VOCM" direction="out"/>
</symbol>
<symbol name="USB-C">
<pin name="CASE"/>
<pin name="CC1"/>
<pin name="CC2"/>
<pin name="D+1"/>
<pin name="D+2"/>
<pin name="D-1"/>
<pin name="D-2"/>
<pin name="GND"/>
<pin name="SBU1"/>
<pin name="SBU2"/>
<pin name="VBUS"/>
</symbol>
<symbol name="STM32G431CB">
<pin name="GND"/>
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA8"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PA15"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PB8-BOOT0"/>
<pin name="PB9"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC4"/>
<pin name="PC6"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC13"/>
<pin name="PC14-OSC32_IN"/>
<pin name="PC15-OSC32_OUT"/>
<pin name="PF0-OSC_IN"/>
<pin name="PF1-OSC_OUT"/>
<pin name="PG10-NRST"/>
<pin name="VBAT"/>
<pin name="VDD"/>
<pin name="VDDA"/>
<pin name="VREF+"/>
</symbol>
<symbol name="SHIELD_4">
<pin name="S1" direction="pas"/>
<pin name="S2" direction="pas"/>
<pin name="S3" direction="pas"/>
<pin name="S4" direction="pas"/>
</symbol>
<symbol name="RFSW6042">
<pin name="ANT"/>
<pin name="C1"/>
<pin name="C2"/>
<pin name="GND"/>
<pin name="RF1"/>
<pin name="RF2"/>
<pin name="RF3"/>
<pin name="RF4"/>
<pin name="VDD"/>
</symbol>
<symbol name="C-EU-1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="MINI-USB-5">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="LOWPASS">
<pin name="GND"/>
<pin name="IN"/>
<pin name="OUT"/>
</symbol>
<symbol name="STW81200SUPPLY">
<pin name="VCC_VCO_CORE" direction="pwr"/>
<pin name="VDD_CP" direction="pwr"/>
<pin name="VCC_CPOUT" direction="pwr"/>
<pin name="VDD_PFD" direction="pwr"/>
<pin name="VDD_DSM_NDIV" direction="pwr"/>
<pin name="VCC_RFOUT" direction="pwr"/>
</symbol>
<symbol name="ADL5801">
<pin name="DETO"/>
<pin name="ENBL"/>
<pin name="GND"/>
<pin name="IN+"/>
<pin name="IN-"/>
<pin name="LO+"/>
<pin name="LO-"/>
<pin name="OUT+"/>
<pin name="OUT-"/>
<pin name="VPDT"/>
<pin name="VPLO"/>
<pin name="VPRF"/>
<pin name="VSET"/>
</symbol>
<symbol name="STW8100LDO">
<pin name="VREG_VCO" direction="out"/>
<pin name="CBYP_4V5" direction="pas"/>
<pin name="VREG_4V5" direction="out"/>
<pin name="CBYP" direction="pas"/>
<pin name="VIN_LDO_VCO" direction="pwr"/>
<pin name="VR" direction="pas"/>
<pin name="VIN_LDO_REF" direction="pwr"/>
<pin name="VREG_REF" direction="out"/>
<pin name="VREG_DIG" direction="out"/>
<pin name="VIN_LDO_RF_DIG" direction="pwr"/>
<pin name="VREG_RF" direction="out"/>
<pin name="VIN_LDO_4V5" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="STW81200RF">
<pin name="VCTRL" direction="in"/>
<pin name="EXTVCO_INP" direction="in"/>
<pin name="EXTVCO_INN" direction="in"/>
<pin name="ICP" direction="out"/>
<pin name="REF_CLKN" direction="in"/>
<pin name="REF_CLKP" direction="in"/>
<pin name="RF1_OUTN"/>
<pin name="RF1_OUTP"/>
<pin name="RF2_OUTN"/>
<pin name="RF2_OUTP"/>
<pin name="HW_PD" direction="in"/>
<pin name="PD_RF1" direction="in"/>
<pin name="PD_RF2/FL_SW" direction="oc"/>
<pin name="LD_SDO" direction="out"/>
<pin name="SDI" direction="in"/>
<pin name="SCK" direction="in"/>
<pin name="LE" direction="in"/>
<pin name="TEST_SE" direction="in"/>
</symbol>
<symbol name="F1958">
<pin name="CLK"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="DATA"/>
<pin name="GND"/>
<pin name="LE"/>
<pin name="MODE"/>
<pin name="RF1"/>
<pin name="RF2"/>
<pin name="VDD"/>
</symbol>
<symbol name="+05V/3">
<pin name="+5V/3" direction="sup"/>
</symbol>
<symbol name="+05V/4">
<pin name="+5V/4" direction="sup"/>
</symbol>
<symbol name="P-MOSFET">
<pin name="S" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="D" direction="pas"/>
</symbol>
<symbol name="PINH2X10">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
<pin name="17" direction="pas" function="dot"/>
<pin name="18" direction="pas" function="dot"/>
<pin name="19" direction="pas" function="dot"/>
<pin name="20" direction="pas" function="dot"/>
</symbol>
<symbol name="LT5560">
<pin name="EN"/>
<pin name="GND"/>
<pin name="IN+"/>
<pin name="IN-"/>
<pin name="LO+"/>
<pin name="LO-"/>
<pin name="OUT+"/>
<pin name="OUT-"/>
<pin name="VCC"/>
</symbol>
<symbol name="C-EU">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="SHIELD">
<pin name="GND"/>
</symbol>
<symbol name="AD9913">
<pin name="PS2/ADR5/D5"/>
<pin name="PS1/ADR4/D4"/>
<pin name="PS0/ADR3/D3"/>
<pin name="DVDD" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="ADR2/D2"/>
<pin name="ADR1/D1"/>
<pin name="ADR0/D0"/>
<pin name="SYNC_CLK" direction="out"/>
<pin name="#SER/PAR" direction="in"/>
<pin name="AGND" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="/REF_CLK" direction="in"/>
<pin name="/IOUT" direction="out"/>
<pin name="IOUT" direction="out"/>
<pin name="RSET" direction="in"/>
<pin name="MASTER_RESET" direction="in"/>
<pin name="PWR_DWN_CTL" direction="in"/>
<pin name="IO_UPDATE" direction="in"/>
<pin name="REF_CLK" direction="in"/>
<pin name="/CS" direction="in"/>
<pin name="SDIO"/>
<pin name="SCLK" direction="in"/>
<pin name="ADR7/D7"/>
<pin name="ADR6/D6"/>
<pin name="EP" direction="pwr"/>
</symbol>
<symbol name="SI5332A-GM1">
<pin name="VDD_DIG" direction="pwr"/>
<pin name="CLKIN_2" direction="in"/>
<pin name="CLKIN_2B" direction="in"/>
<pin name="VDD_XTAL" direction="pwr"/>
<pin name="XA/CLKIN1" direction="in"/>
<pin name="VDDA" direction="pwr"/>
<pin name="INPUT1" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="SDA"/>
<pin name="OUT0B" direction="out"/>
<pin name="OUT0" direction="out"/>
<pin name="VDDO0" direction="pwr"/>
<pin name="OUT1B" direction="out"/>
<pin name="OUT1" direction="out"/>
<pin name="VDDO1" direction="pwr"/>
<pin name="INPUT2" direction="in"/>
<pin name="OUT2B" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="VDDO2" direction="pwr"/>
<pin name="OUT3B" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="VDDO3" direction="pwr"/>
<pin name="INPUT3" direction="in"/>
<pin name="VDDO4" direction="pwr"/>
<pin name="OUT4B" direction="out"/>
<pin name="OUT4" direction="out"/>
<pin name="INPUT4" direction="in"/>
<pin name="INPUT5" direction="in"/>
<pin name="OUT5B" direction="out"/>
<pin name="OUT5" direction="out"/>
<pin name="VDDO5" direction="pwr"/>
<pin name="GND"/>
<pin name="XB" direction="in"/>
</symbol>
<symbol name="STM32L462CE">
<pin name="VBAT" direction="pwr"/>
<pin name="PC13"/>
<pin name="PC14-OSC32_IN"/>
<pin name="PC15-OSC32_OUT"/>
<pin name="PH0-OSC_IN"/>
<pin name="PH1_OSC_OUT"/>
<pin name="NRST" direction="in"/>
<pin name="VSSA/VREF-" direction="pwr"/>
<pin name="VDDA/VREF+" direction="pwr"/>
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA3"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PA8"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PA13/SWDIO"/>
<pin name="VDDUSB"/>
<pin name="PA14/SWCLK"/>
<pin name="PA15"/>
<pin name="EP"/>
<pin name="PB9"/>
<pin name="PB8"/>
<pin name="PH3-BOOT0"/>
<pin name="PB7"/>
<pin name="PB6"/>
<pin name="PB5"/>
<pin name="PB4"/>
<pin name="PB3"/>
<pin name="PB2"/>
</symbol>
<symbol name="ATTENUATOR_3PIN">
<pin name="IN"/>
<pin name="OUT"/>
<pin name="GND"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="GND" prefix="GND">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="GND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="+5V/1" prefix="SUPPLY">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="+05V/1"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VCCINT" prefix="VCC">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="VCCINT"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="+5V/2" prefix="SUPPLY">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="+05V/2"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="A3L-LOC" prefix="FRAME" uservalue="yes">
<description>&lt;b&gt;FRAME&lt;/b&gt;&lt;p&gt;
DIN A3, landscape with location and doc. field</description>
<gates>
<gate name="G$1" symbol="A3L-LOC"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="+3V3" prefix="+3V3">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="+3V3"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="+12V" prefix="SUPPLY">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="+12V" symbol="+12V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="+5V/4" prefix="SUPPLY">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="+05V/4"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="+5V/3" prefix="SUPPLY">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="+05V/3"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="QPC6324" prefix="IC">
<gates>
<gate name="G$1" symbol="QPC6324"/>
</gates>
<devices>
<device name="" package="QFN50P400X400X75-21T206">
<connects>
<connect gate="G$1" pin="CTL1" pad="17"/>
<connect gate="G$1" pin="CTL2" pad="16"/>
<connect gate="G$1" pin="GND" pad="1 2 4 5 6 7 9 10 11 12 14 15 18 19 21"/>
<connect gate="G$1" pin="RF1" pad="3"/>
<connect gate="G$1" pin="RF2" pad="13"/>
<connect gate="G$1" pin="RF_COM" pad="8"/>
<connect gate="G$1" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SI5351C" prefix="IC">
<gates>
<gate name="G$1" symbol="SI5351C"/>
</gates>
<devices>
<device name="" package="QFN50P400X400X90-21T270N">
<connects>
<connect gate="G$1" pin="CLK0" pad="13"/>
<connect gate="G$1" pin="CLK1" pad="12"/>
<connect gate="G$1" pin="CLK2" pad="9"/>
<connect gate="G$1" pin="CLK3" pad="8"/>
<connect gate="G$1" pin="CLK4" pad="19"/>
<connect gate="G$1" pin="CLK5" pad="17"/>
<connect gate="G$1" pin="CLK6" pad="16"/>
<connect gate="G$1" pin="CLK7" pad="15"/>
<connect gate="G$1" pin="CLKIN" pad="6"/>
<connect gate="G$1" pin="GND" pad="21"/>
<connect gate="G$1" pin="INTR" pad="3"/>
<connect gate="G$1" pin="OEB" pad="7"/>
<connect gate="G$1" pin="SCL" pad="4"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VDDOA" pad="11"/>
<connect gate="G$1" pin="VDDOB" pad="10"/>
<connect gate="G$1" pin="VDDOC" pad="18"/>
<connect gate="G$1" pin="VDDOD" pad="14"/>
<connect gate="G$1" pin="XA" pad="1"/>
<connect gate="G$1" pin="XB" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3370" prefix="IC">
<gates>
<gate name="BUCK1" symbol="LM3370_BUCK"/>
<gate name="BUCK2" symbol="LM3370_BUCK"/>
<gate name="CONTROL" symbol="LM3370_CONTROL"/>
</gates>
<devices>
<device name="" package="SON50P400X500X80-17T260X400N">
<connects>
<connect gate="BUCK1" pin="/POR" pad="12"/>
<connect gate="BUCK1" pin="EN" pad="14"/>
<connect gate="BUCK1" pin="FB" pad="9"/>
<connect gate="BUCK1" pin="PGND" pad="6"/>
<connect gate="BUCK1" pin="SW" pad="7"/>
<connect gate="BUCK1" pin="VIN" pad="8"/>
<connect gate="BUCK2" pin="/POR" pad="13"/>
<connect gate="BUCK2" pin="EN" pad="15"/>
<connect gate="BUCK2" pin="FB" pad="16"/>
<connect gate="BUCK2" pin="PGND" pad="3"/>
<connect gate="BUCK2" pin="SW" pad="2"/>
<connect gate="BUCK2" pin="VIN" pad="1"/>
<connect gate="CONTROL" pin="SCL" pad="11"/>
<connect gate="CONTROL" pin="SDA" pad="10"/>
<connect gate="CONTROL" pin="SGND" pad="5 17"/>
<connect gate="CONTROL" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="W25Q16BV" prefix="U">
<description>&lt;b&gt;EEPROM&lt;/b&gt;&lt;p&gt;
4 Mbit SPI Serial Flash7</description>
<gates>
<gate name="G$1" symbol="25XX"/>
</gates>
<devices>
<device name="SN" package="SO08">
<connects>
<connect gate="G$1" pin="!CS!" pad="1"/>
<connect gate="G$1" pin="!HOLD!" pad="7"/>
<connect gate="G$1" pin="!WP!" pad="3"/>
<connect gate="G$1" pin="CLK" pad="6"/>
<connect gate="G$1" pin="DI" pad="5"/>
<connect gate="G$1" pin="DO" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP33131D-10-E/MS" prefix="IC">
<gates>
<gate name="G$1" symbol="MCP33131D-10-E/MS"/>
</gates>
<devices>
<device name="" package="SOP50P490X110-10N">
<connects>
<connect gate="G$1" pin="AIN+" pad="3"/>
<connect gate="G$1" pin="AIN-" pad="4"/>
<connect gate="G$1" pin="AVDD" pad="2"/>
<connect gate="G$1" pin="CONVST" pad="6"/>
<connect gate="G$1" pin="DVIO" pad="10"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="SCLK" pad="8"/>
<connect gate="G$1" pin="SDI" pad="9"/>
<connect gate="G$1" pin="SDO" pad="7"/>
<connect gate="G$1" pin="VREF" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SMA_CONNECTOR" prefix="X">
<gates>
<gate name="G$1" symbol="BNC-FGND"/>
</gates>
<devices>
<device name="" package="J502-ND-142-0711-821/826">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="G@1 G@2 G@3 G@4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX2871" prefix="IC">
<gates>
<gate name="G$1" symbol="MAX2871"/>
</gates>
<devices>
<device name="" package="QFN50P500X500X80-33T310">
<connects>
<connect gate="G$1" pin="BIAS_FILT" pad="23"/>
<connect gate="G$1" pin="CE" pad="4"/>
<connect gate="G$1" pin="CLK" pad="1"/>
<connect gate="G$1" pin="CP_OUT" pad="7"/>
<connect gate="G$1" pin="DATA" pad="2"/>
<connect gate="G$1" pin="EP" pad="33"/>
<connect gate="G$1" pin="GND_CP" pad="8"/>
<connect gate="G$1" pin="GND_DIG" pad="27"/>
<connect gate="G$1" pin="GND_PLL" pad="9"/>
<connect gate="G$1" pin="GND_RF" pad="11"/>
<connect gate="G$1" pin="GND_SD" pad="31"/>
<connect gate="G$1" pin="GND_TUNE" pad="21"/>
<connect gate="G$1" pin="GND_VCO" pad="18"/>
<connect gate="G$1" pin="LD" pad="25"/>
<connect gate="G$1" pin="LE" pad="3"/>
<connect gate="G$1" pin="MUX" pad="30"/>
<connect gate="G$1" pin="NOISE_FILT" pad="19"/>
<connect gate="G$1" pin="REF_IN" pad="29"/>
<connect gate="G$1" pin="REG" pad="24"/>
<connect gate="G$1" pin="RFOUTA_N" pad="13"/>
<connect gate="G$1" pin="RFOUTA_P" pad="12"/>
<connect gate="G$1" pin="RFOUTB_N" pad="15"/>
<connect gate="G$1" pin="RFOUTB_P" pad="14"/>
<connect gate="G$1" pin="RFOUT_EN" pad="26"/>
<connect gate="G$1" pin="RSET" pad="22"/>
<connect gate="G$1" pin="SW" pad="5"/>
<connect gate="G$1" pin="TUNE" pad="20"/>
<connect gate="G$1" pin="VCC_CP" pad="6"/>
<connect gate="G$1" pin="VCC_DIG" pad="28"/>
<connect gate="G$1" pin="VCC_PLL" pad="10"/>
<connect gate="G$1" pin="VCC_RF" pad="16"/>
<connect gate="G$1" pin="VCC_VCO" pad="17"/>
<connect gate="G$1" pin="VDD_SD" pad="32"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FA-" prefix="Q">
<description>&lt;b&gt;MHz RANGE CRYSTAL UNIT&lt;/b&gt; &lt;p&gt;
Source: Epson Toyocom</description>
<gates>
<gate name="G$1" symbol="Q-SHIELD2"/>
</gates>
<devices>
<device name="128" package="FA-128">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP702" prefix="IC">
<gates>
<gate name="G$1" symbol="VREG_EN"/>
</gates>
<devices>
<device name="" package="SOT95P240X110-5">
<connects>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SRN5040" prefix="L">
<gates>
<gate name="G$1" symbol="L-EU"/>
</gates>
<devices>
<device name="" package="SRN5040">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INDUCTOR" prefix="L">
<gates>
<gate name="G$1" symbol="L-EU:1"/>
</gates>
<devices>
<device name="0402" package="L0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="INDC2012X100N">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R-EU_" prefix="R" uservalue="yes">
<description>&lt;B&gt;RESISTOR&lt;/B&gt;, European symbol</description>
<gates>
<gate name="G$1" symbol="R-EU"/>
</gates>
<devices>
<device name="R0402" package="R0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FERRITE" prefix="L">
<gates>
<gate name="G$1" symbol="L-EU:1"/>
</gates>
<devices>
<device name="" package="R0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRF37A73" prefix="IC">
<gates>
<gate name="G$1" symbol="AMPLIFIER_PWDN"/>
</gates>
<devices>
<device name="" package="SON50P200X200X80-9T90X160N">
<connects>
<connect gate="G$1" pin="GND" pad="3 4 6 8 9"/>
<connect gate="G$1" pin="PWDN" pad="5"/>
<connect gate="G$1" pin="RFIN" pad="2"/>
<connect gate="G$1" pin="RFOUT" pad="7"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TP" prefix="TP">
<description>&lt;b&gt;Test pad&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="TP"/>
</gates>
<devices>
<device name="B1,27" package="B1,27">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DCJ0202" prefix="J">
<description>&lt;b&gt;DC POWER JACK&lt;/b&gt;&lt;p&gt;
Source: DCJ0202.pdf</description>
<gates>
<gate name="G$1" symbol="DC-JACK-SWITCH"/>
</gates>
<devices>
<device name="" package="DCJ0202">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED" prefix="LED" uservalue="yes">
<description>&lt;b&gt;LED&lt;/b&gt;&lt;p&gt;
&lt;u&gt;OSRAM&lt;/u&gt;:&lt;br&gt;

- &lt;u&gt;CHIPLED&lt;/u&gt;&lt;br&gt;
LG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971
LH N974, LH R974&lt;br&gt;
LS Q976, LO Q976, LY Q976&lt;br&gt;
LO Q996&lt;br&gt;

- &lt;u&gt;Hyper CHIPLED&lt;/u&gt;&lt;br&gt;
LW Q18S&lt;br&gt;
LB Q993, LB Q99A, LB R99A&lt;br&gt;

- &lt;u&gt;SideLED&lt;/u&gt;&lt;br&gt;
LS A670, LO A670, LY A670, LG A670, LP A670&lt;br&gt;
LB A673, LV A673, LT A673, LW A673&lt;br&gt;
LH A674&lt;br&gt;
LY A675&lt;br&gt;
LS A676, LA A676, LO A676, LY A676, LW A676&lt;br&gt;
LS A679, LY A679, LG A679&lt;br&gt;

-  &lt;u&gt;Hyper Micro SIDELED®&lt;/u&gt;&lt;br&gt;
LS Y876, LA Y876, LO Y876, LY Y876&lt;br&gt;
LT Y87S&lt;br&gt;

- &lt;u&gt;SmartLED&lt;/u&gt;&lt;br&gt;
LW L88C, LW L88S&lt;br&gt;
LB L89C, LB L89S, LG L890&lt;br&gt;
LS L89K, LO L89K, LY L89K&lt;br&gt;
LS L896, LA L896, LO L896, LY L896&lt;br&gt;

- &lt;u&gt;TOPLED&lt;/u&gt;&lt;br&gt;
LS T670, LO T670, LY T670, LG T670, LP T670&lt;br&gt;
LSG T670, LSP T670, LSY T670, LOP T670, LYG T670&lt;br&gt;
LG T671, LOG T671, LSG T671&lt;br&gt;
LB T673, LV T673, LT T673, LW T673&lt;br&gt;
LH T674&lt;br&gt;
LS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676&lt;br&gt;
LB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C&lt;br&gt;
LS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C&lt;br&gt;
LW T67C&lt;br&gt;
LS T679, LY T679, LG T679&lt;br&gt;
LS T770, LO T770, LY T770, LG T770, LP T770&lt;br&gt;
LB T773, LV T773, LT T773, LW T773&lt;br&gt;
LH T774&lt;br&gt;
LS E675, LA E675, LY E675, LS T675&lt;br&gt;
LS T776, LA T776, LO T776, LY T776, LB T776&lt;br&gt;
LHGB T686&lt;br&gt;
LT T68C, LB T68C&lt;br&gt;

- &lt;u&gt;Hyper Mini TOPLED®&lt;/u&gt;&lt;br&gt;
LB M676&lt;br&gt;

- &lt;u&gt;Mini TOPLED Santana®&lt;/u&gt;&lt;br&gt;
LG M470&lt;br&gt;
LS M47K, LO M47K, LY M47K
&lt;p&gt;
Source: http://www.osram.convergy.de&lt;p&gt;

&lt;u&gt;LUXEON:&lt;/u&gt;&lt;br&gt;
- &lt;u&gt;LUMILED®&lt;/u&gt;&lt;br&gt;
LXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00&lt;br&gt;
LXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00&lt;br&gt;
LXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00&lt;br&gt;
LXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00&lt;br&gt;
LXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00&lt;br&gt;
LXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00&lt;br&gt;
LXK2-PH12-R00, LXK2-PH12-S00&lt;br&gt;
LXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00
&lt;p&gt;
Source: www.luxeon.com&lt;p&gt;

&lt;u&gt;KINGBRIGHT:&lt;/U&gt;&lt;p&gt;
KA-3528ASYC&lt;br&gt;
Source: www.kingbright.com</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="CHIPLED_0603" package="CHIPLED_0603">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="POPULARITY" value="0"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="D-" prefix="D" uservalue="yes">
<description>&lt;B&gt;DIODE&lt;/B&gt;</description>
<gates>
<gate name="G$1" symbol="D"/>
</gates>
<devices>
<device name="SMB" package="SMB">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPS65265" prefix="IC">
<gates>
<gate name="COMMON" symbol="TPS65265COM"/>
<gate name="G1" symbol="TPS65265BUCK"/>
<gate name="G2" symbol="TPS65265BUCK"/>
<gate name="G3" symbol="TPS65265BUCK"/>
</gates>
<devices>
<device name="" package="QFN50P500X500X100-33T345N">
<connects>
<connect gate="COMMON" pin="AGND" pad="21 33"/>
<connect gate="COMMON" pin="MODE" pad="8"/>
<connect gate="COMMON" pin="PGOOD" pad="2"/>
<connect gate="COMMON" pin="PG_DLY" pad="24"/>
<connect gate="COMMON" pin="PSM" pad="32"/>
<connect gate="COMMON" pin="ROSC" pad="20"/>
<connect gate="COMMON" pin="SEQ_DLY" pad="17"/>
<connect gate="COMMON" pin="V7V" pad="1"/>
<connect gate="G1" pin="BST" pad="25"/>
<connect gate="G1" pin="COMP" pad="23"/>
<connect gate="G1" pin="EN" pad="3"/>
<connect gate="G1" pin="FB" pad="22"/>
<connect gate="G1" pin="GND" pad="26 27"/>
<connect gate="G1" pin="LX" pad="28 29"/>
<connect gate="G1" pin="VIN" pad="30 31"/>
<connect gate="G2" pin="BST" pad="9"/>
<connect gate="G2" pin="COMP" pad="7"/>
<connect gate="G2" pin="EN" pad="4"/>
<connect gate="G2" pin="FB" pad="6"/>
<connect gate="G2" pin="GND" pad="10"/>
<connect gate="G2" pin="LX" pad="11"/>
<connect gate="G2" pin="VIN" pad="12"/>
<connect gate="G3" pin="BST" pad="16"/>
<connect gate="G3" pin="COMP" pad="18"/>
<connect gate="G3" pin="EN" pad="5"/>
<connect gate="G3" pin="FB" pad="19"/>
<connect gate="G3" pin="GND" pad="15"/>
<connect gate="G3" pin="LX" pad="14"/>
<connect gate="G3" pin="VIN" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AP2114" prefix="IC">
<gates>
<gate name="G$1" symbol="VREG"/>
</gates>
<devices>
<device name="H" package="SOT230P700X180-4">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VIN" pad="3"/>
<connect gate="G$1" pin="VOUT" pad="2 4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HA" package="SOT230P700X180-4">
<connects>
<connect gate="G$1" pin="GND" pad="2 4"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="C-EU*?:2" prefix="C" uservalue="yes">
<description>&lt;B&gt;CAPACITOR&lt;/B&gt;, European symbol</description>
<gates>
<gate name="G$1" symbol="C-EU:1"/>
</gates>
<devices>
<device name="C0402" package="C0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AMPHENOL_132289" prefix="J">
<gates>
<gate name="G$1" symbol="COAX"/>
</gates>
<devices>
<device name="" package="AMPHENOL_132289">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="G@1 G@2 G@3 G@4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X10" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD10"/>
</gates>
<devices>
<device name="/90" package="1X10/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NFM18CC101R1C3D" prefix="C">
<gates>
<gate name="G$1" symbol="C-FILTER"/>
</gates>
<devices>
<device name="" package="NFM18PC">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2@1" pad="2"/>
<connect gate="G$1" pin="2@2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NFM21PC475B1A3D" prefix="C">
<gates>
<gate name="G$1" symbol="C-FILTER"/>
</gates>
<devices>
<device name="" package="NFM21PC">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2@1" pad="2" route="any"/>
<connect gate="G$1" pin="2@2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="THS4521IDGKR" prefix="IC">
<gates>
<gate name="G$1" symbol="OPAMPDIFF_SHDN"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="G$1" pin="+IN" pad="8"/>
<connect gate="G$1" pin="+OUT" pad="4"/>
<connect gate="G$1" pin="-IN" pad="1"/>
<connect gate="G$1" pin="-OUT" pad="5"/>
<connect gate="G$1" pin="SHDN" pad="7"/>
<connect gate="G$1" pin="V+" pad="3"/>
<connect gate="G$1" pin="V-" pad="6"/>
<connect gate="G$1" pin="VOCM" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MIC2253" prefix="IC">
<gates>
<gate name="G$1" symbol="MIC2253"/>
</gates>
<devices>
<device name="" package="SON50P300X300X90-13T170X240N">
<connects>
<connect gate="G$1" pin="AGND" pad="4"/>
<connect gate="G$1" pin="COMP" pad="12"/>
<connect gate="G$1" pin="EN" pad="11"/>
<connect gate="G$1" pin="FB" pad="3"/>
<connect gate="G$1" pin="OVP" pad="9"/>
<connect gate="G$1" pin="PGND" pad="5 6 13"/>
<connect gate="G$1" pin="SS" pad="2"/>
<connect gate="G$1" pin="SW" pad="7 8"/>
<connect gate="G$1" pin="VIN" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="B012-617DB-1-63-B331" prefix="T">
<gates>
<gate name="G$1" symbol="BALUN_1:1"/>
</gates>
<devices>
<device name="" package="EASTEVER_BALUN">
<connects>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="2"/>
<connect gate="G$1" pin="OUT+" pad="4"/>
<connect gate="G$1" pin="OUT-" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LDL212PU50R" prefix="IC">
<gates>
<gate name="G$1" symbol="LDL212"/>
</gates>
<devices>
<device name="" package="SON95P300X300X100-7T170X240N">
<connects>
<connect gate="G$1" pin="EN" pad="6"/>
<connect gate="G$1" pin="GND" pad="1 7"/>
<connect gate="G$1" pin="SENSE" pad="2"/>
<connect gate="G$1" pin="VIN" pad="4"/>
<connect gate="G$1" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6SLX9TQG144" prefix="U">
<description>Xilinx FPGA: 6SLX9TQG144</description>
<gates>
<gate name="B0" symbol="6SLX9TQG144_0"/>
<gate name="B1" symbol="6SLX9TQG144_1"/>
<gate name="B2" symbol="6SLX9TQG144_2"/>
<gate name="B3" symbol="6SLX9TQG144_3"/>
<gate name="BGND" symbol="6SLX9TQG144_GND"/>
<gate name="BNA" symbol="6SLX9TQG144_NA"/>
<gate name="BVCCAUX" symbol="6SLX9TQG144_VCCAUX"/>
<gate name="BVCCINT" symbol="6SLX9TQG144_VCCINT"/>
</gates>
<devices>
<device name="" package="TQ144">
<connects>
<connect gate="B0" pin="IO_L1N_VREF_0" pad="P143"/>
<connect gate="B0" pin="IO_L1P_HSWAPEN_0" pad="P144"/>
<connect gate="B0" pin="IO_L2N_0" pad="P141"/>
<connect gate="B0" pin="IO_L2P_0" pad="P142"/>
<connect gate="B0" pin="IO_L34N_GCLK18_0" pad="P133"/>
<connect gate="B0" pin="IO_L34P_GCLK19_0" pad="P134"/>
<connect gate="B0" pin="IO_L35N_GCLK16_0" pad="P131"/>
<connect gate="B0" pin="IO_L35P_GCLK17_0" pad="P132"/>
<connect gate="B0" pin="IO_L36N_GCLK14_0" pad="P126"/>
<connect gate="B0" pin="IO_L36P_GCLK15_0" pad="P127"/>
<connect gate="B0" pin="IO_L37N_GCLK12_0" pad="P123"/>
<connect gate="B0" pin="IO_L37P_GCLK13_0" pad="P124"/>
<connect gate="B0" pin="IO_L3N_0" pad="P139"/>
<connect gate="B0" pin="IO_L3P_0" pad="P140"/>
<connect gate="B0" pin="IO_L4N_0" pad="P137"/>
<connect gate="B0" pin="IO_L4P_0" pad="P138"/>
<connect gate="B0" pin="IO_L62N_VREF_0" pad="P120"/>
<connect gate="B0" pin="IO_L62P_0" pad="P121"/>
<connect gate="B0" pin="IO_L63N_SCP6_0" pad="P118"/>
<connect gate="B0" pin="IO_L63P_SCP7_0" pad="P119"/>
<connect gate="B0" pin="IO_L64N_SCP4_0" pad="P116"/>
<connect gate="B0" pin="IO_L64P_SCP5_0" pad="P117"/>
<connect gate="B0" pin="IO_L65N_SCP2_0" pad="P114"/>
<connect gate="B0" pin="IO_L65P_SCP3_0" pad="P115"/>
<connect gate="B0" pin="IO_L66N_SCP0_0" pad="P111"/>
<connect gate="B0" pin="IO_L66P_SCP1_0" pad="P112"/>
<connect gate="B0" pin="VCCO_0@0" pad="P122"/>
<connect gate="B0" pin="VCCO_0@1" pad="P125"/>
<connect gate="B0" pin="VCCO_0@2" pad="P135"/>
<connect gate="B1" pin="IO_L1N_VREF_1" pad="P104"/>
<connect gate="B1" pin="IO_L1P_1" pad="P105"/>
<connect gate="B1" pin="IO_L32N_1" pad="P101"/>
<connect gate="B1" pin="IO_L32P_1" pad="P102"/>
<connect gate="B1" pin="IO_L33N_1" pad="P99"/>
<connect gate="B1" pin="IO_L33P_1" pad="P100"/>
<connect gate="B1" pin="IO_L34N_1" pad="P97"/>
<connect gate="B1" pin="IO_L34P_1" pad="P98"/>
<connect gate="B1" pin="IO_L40N_GCLK10_1" pad="P94"/>
<connect gate="B1" pin="IO_L40P_GCLK11_1" pad="P95"/>
<connect gate="B1" pin="IO_L41N_GCLK8_1" pad="P92"/>
<connect gate="B1" pin="IO_L41P_GCLK9_IRDY1_1" pad="P93"/>
<connect gate="B1" pin="IO_L42N_GCLK6_TRDY1_1" pad="P87"/>
<connect gate="B1" pin="IO_L42P_GCLK7_1" pad="P88"/>
<connect gate="B1" pin="IO_L43N_GCLK4_1" pad="P84"/>
<connect gate="B1" pin="IO_L43P_GCLK5_1" pad="P85"/>
<connect gate="B1" pin="IO_L45N_1" pad="P82"/>
<connect gate="B1" pin="IO_L45P_1" pad="P83"/>
<connect gate="B1" pin="IO_L46N_1" pad="P80"/>
<connect gate="B1" pin="IO_L46P_1" pad="P81"/>
<connect gate="B1" pin="IO_L47N_1" pad="P78"/>
<connect gate="B1" pin="IO_L47P_1" pad="P79"/>
<connect gate="B1" pin="IO_L74N_DOUT_BUSY_1" pad="P74"/>
<connect gate="B1" pin="IO_L74P_AWAKE_1" pad="P75"/>
<connect gate="B1" pin="VCCO_1@0" pad="P76"/>
<connect gate="B1" pin="VCCO_1@1" pad="P86"/>
<connect gate="B1" pin="VCCO_1@2" pad="P103"/>
<connect gate="B2" pin="CMPCS_B_2" pad="P72"/>
<connect gate="B2" pin="DONE_2" pad="P71"/>
<connect gate="B2" pin="IO_L12N_D2_MISO3_2" pad="P61"/>
<connect gate="B2" pin="IO_L12P_D1_MISO2_2" pad="P62"/>
<connect gate="B2" pin="IO_L13N_D10_2" pad="P59"/>
<connect gate="B2" pin="IO_L13P_M1_2" pad="P60"/>
<connect gate="B2" pin="IO_L14N_D12_2" pad="P57"/>
<connect gate="B2" pin="IO_L14P_D11_2" pad="P58"/>
<connect gate="B2" pin="IO_L1N_M0_CMPMISO_2" pad="P69"/>
<connect gate="B2" pin="IO_L1P_CCLK_2" pad="P70"/>
<connect gate="B2" pin="IO_L2N_CMPMOSI_2" pad="P66"/>
<connect gate="B2" pin="IO_L2P_CMPCLK_2" pad="P67"/>
<connect gate="B2" pin="IO_L30N_GCLK0_USERCCLK_2" pad="P55"/>
<connect gate="B2" pin="IO_L30P_GCLK1_D13_2" pad="P56"/>
<connect gate="B2" pin="IO_L31N_GCLK30_D15_2" pad="P50"/>
<connect gate="B2" pin="IO_L31P_GCLK31_D14_2" pad="P51"/>
<connect gate="B2" pin="IO_L3N_MOSI_CSI_B_MISO0_2" pad="P64"/>
<connect gate="B2" pin="IO_L3P_D0_DIN_MISO_MISO1_2" pad="P65"/>
<connect gate="B2" pin="IO_L48N_RDWR_B_VREF_2" pad="P47"/>
<connect gate="B2" pin="IO_L48P_D7_2" pad="P48"/>
<connect gate="B2" pin="IO_L49N_D4_2" pad="P45"/>
<connect gate="B2" pin="IO_L49P_D3_2" pad="P46"/>
<connect gate="B2" pin="IO_L62N_D6_2" pad="P43"/>
<connect gate="B2" pin="IO_L62P_D5_2" pad="P44"/>
<connect gate="B2" pin="IO_L64N_D9_2" pad="P40"/>
<connect gate="B2" pin="IO_L64P_D8_2" pad="P41"/>
<connect gate="B2" pin="IO_L65N_CSO_B_2" pad="P38"/>
<connect gate="B2" pin="IO_L65P_INIT_B_2" pad="P39"/>
<connect gate="B2" pin="PROGRAM_B_2" pad="P37"/>
<connect gate="B2" pin="VCCO_2@0" pad="P42"/>
<connect gate="B2" pin="VCCO_2@1" pad="P63"/>
<connect gate="B3" pin="IO_L1N_VREF_3" pad="P34"/>
<connect gate="B3" pin="IO_L1P_3" pad="P35"/>
<connect gate="B3" pin="IO_L2N_3" pad="P32"/>
<connect gate="B3" pin="IO_L2P_3" pad="P33"/>
<connect gate="B3" pin="IO_L36N_3" pad="P29"/>
<connect gate="B3" pin="IO_L36P_3" pad="P30"/>
<connect gate="B3" pin="IO_L37N_3" pad="P26"/>
<connect gate="B3" pin="IO_L37P_3" pad="P27"/>
<connect gate="B3" pin="IO_L41N_GCLK26_3" pad="P23"/>
<connect gate="B3" pin="IO_L41P_GCLK27_3" pad="P24"/>
<connect gate="B3" pin="IO_L42N_GCLK24_3" pad="P21"/>
<connect gate="B3" pin="IO_L42P_GCLK25_TRDY2_3" pad="P22"/>
<connect gate="B3" pin="IO_L43N_GCLK22_IRDY2_3" pad="P16"/>
<connect gate="B3" pin="IO_L43P_GCLK23_3" pad="P17"/>
<connect gate="B3" pin="IO_L44N_GCLK20_3" pad="P14"/>
<connect gate="B3" pin="IO_L44P_GCLK21_3" pad="P15"/>
<connect gate="B3" pin="IO_L49N_3" pad="P11"/>
<connect gate="B3" pin="IO_L49P_3" pad="P12"/>
<connect gate="B3" pin="IO_L50N_3" pad="P9"/>
<connect gate="B3" pin="IO_L50P_3" pad="P10"/>
<connect gate="B3" pin="IO_L51N_3" pad="P7"/>
<connect gate="B3" pin="IO_L51P_3" pad="P8"/>
<connect gate="B3" pin="IO_L52N_3" pad="P5"/>
<connect gate="B3" pin="IO_L52P_3" pad="P6"/>
<connect gate="B3" pin="IO_L83N_VREF_3" pad="P1"/>
<connect gate="B3" pin="IO_L83P_3" pad="P2"/>
<connect gate="B3" pin="VCCO_3@0" pad="P4"/>
<connect gate="B3" pin="VCCO_3@1" pad="P18"/>
<connect gate="B3" pin="VCCO_3@2" pad="P31"/>
<connect gate="BGND" pin="GND@0" pad="P3"/>
<connect gate="BGND" pin="GND@1" pad="P13"/>
<connect gate="BGND" pin="GND@10" pad="P113"/>
<connect gate="BGND" pin="GND@11" pad="P130"/>
<connect gate="BGND" pin="GND@12" pad="P136"/>
<connect gate="BGND" pin="GND@2" pad="P25"/>
<connect gate="BGND" pin="GND@3" pad="P49"/>
<connect gate="BGND" pin="GND@4" pad="P54"/>
<connect gate="BGND" pin="GND@5" pad="P68"/>
<connect gate="BGND" pin="GND@6" pad="P77"/>
<connect gate="BGND" pin="GND@7" pad="P91"/>
<connect gate="BGND" pin="GND@8" pad="P96"/>
<connect gate="BGND" pin="GND@9" pad="P108"/>
<connect gate="BNA" pin="SUSPEND" pad="P73"/>
<connect gate="BNA" pin="TCK" pad="P109"/>
<connect gate="BNA" pin="TDI" pad="P110"/>
<connect gate="BNA" pin="TDO" pad="P106"/>
<connect gate="BNA" pin="TMS" pad="P107"/>
<connect gate="BVCCAUX" pin="VCCAUX@0" pad="P20"/>
<connect gate="BVCCAUX" pin="VCCAUX@1" pad="P36"/>
<connect gate="BVCCAUX" pin="VCCAUX@2" pad="P53"/>
<connect gate="BVCCAUX" pin="VCCAUX@3" pad="P90"/>
<connect gate="BVCCAUX" pin="VCCAUX@4" pad="P129"/>
<connect gate="BVCCINT" pin="VCCINT@0" pad="P19"/>
<connect gate="BVCCINT" pin="VCCINT@1" pad="P28"/>
<connect gate="BVCCINT" pin="VCCINT@2" pad="P52"/>
<connect gate="BVCCINT" pin="VCCINT@3" pad="P89"/>
<connect gate="BVCCINT" pin="VCCINT@4" pad="P128"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="C-EU*?:1" prefix="C" uservalue="yes">
<description>&lt;B&gt;CAPACITOR&lt;/B&gt;, European symbol</description>
<gates>
<gate name="G$1" symbol="C-EU-1"/>
</gates>
<devices>
<device name="C0603" package="C0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TYPE-C16P(073)" prefix="J">
<gates>
<gate name="G$1" symbol="USB-C"/>
</gates>
<devices>
<device name="" package="TYPE-C16P">
<connects>
<connect gate="G$1" pin="CASE" pad="M1 M2 M3 M4"/>
<connect gate="G$1" pin="CC1" pad="4"/>
<connect gate="G$1" pin="CC2" pad="10"/>
<connect gate="G$1" pin="D+1" pad="6"/>
<connect gate="G$1" pin="D+2" pad="8"/>
<connect gate="G$1" pin="D-1" pad="7"/>
<connect gate="G$1" pin="D-2" pad="5"/>
<connect gate="G$1" pin="GND" pad="1 12"/>
<connect gate="G$1" pin="SBU1" pad="9"/>
<connect gate="G$1" pin="SBU2" pad="3"/>
<connect gate="G$1" pin="VBUS" pad="2 11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32G431CB" prefix="IC">
<gates>
<gate name="G$1" symbol="STM32G431CB"/>
</gates>
<devices>
<device name="" package="QFN50P700X700X60-49T560N">
<connects>
<connect gate="G$1" pin="GND" pad="49"/>
<connect gate="G$1" pin="PA0" pad="8"/>
<connect gate="G$1" pin="PA1" pad="9"/>
<connect gate="G$1" pin="PA10" pad="32"/>
<connect gate="G$1" pin="PA11" pad="33"/>
<connect gate="G$1" pin="PA12" pad="34"/>
<connect gate="G$1" pin="PA13" pad="36"/>
<connect gate="G$1" pin="PA14" pad="37"/>
<connect gate="G$1" pin="PA15" pad="38"/>
<connect gate="G$1" pin="PA2" pad="10"/>
<connect gate="G$1" pin="PA3" pad="11"/>
<connect gate="G$1" pin="PA4" pad="12"/>
<connect gate="G$1" pin="PA5" pad="13"/>
<connect gate="G$1" pin="PA6" pad="14"/>
<connect gate="G$1" pin="PA7" pad="15"/>
<connect gate="G$1" pin="PA8" pad="30"/>
<connect gate="G$1" pin="PA9" pad="31"/>
<connect gate="G$1" pin="PB0" pad="17"/>
<connect gate="G$1" pin="PB1" pad="18"/>
<connect gate="G$1" pin="PB10" pad="22"/>
<connect gate="G$1" pin="PB11" pad="24"/>
<connect gate="G$1" pin="PB12" pad="25"/>
<connect gate="G$1" pin="PB13" pad="26"/>
<connect gate="G$1" pin="PB14" pad="27"/>
<connect gate="G$1" pin="PB15" pad="28"/>
<connect gate="G$1" pin="PB2" pad="19"/>
<connect gate="G$1" pin="PB3" pad="41"/>
<connect gate="G$1" pin="PB4" pad="42"/>
<connect gate="G$1" pin="PB5" pad="43"/>
<connect gate="G$1" pin="PB6" pad="44"/>
<connect gate="G$1" pin="PB7" pad="45"/>
<connect gate="G$1" pin="PB8-BOOT0" pad="46"/>
<connect gate="G$1" pin="PB9" pad="47"/>
<connect gate="G$1" pin="PC10" pad="39"/>
<connect gate="G$1" pin="PC11" pad="40"/>
<connect gate="G$1" pin="PC13" pad="2"/>
<connect gate="G$1" pin="PC14-OSC32_IN" pad="3"/>
<connect gate="G$1" pin="PC15-OSC32_OUT" pad="4"/>
<connect gate="G$1" pin="PC4" pad="16"/>
<connect gate="G$1" pin="PC6" pad="29"/>
<connect gate="G$1" pin="PF0-OSC_IN" pad="5"/>
<connect gate="G$1" pin="PF1-OSC_OUT" pad="6"/>
<connect gate="G$1" pin="PG10-NRST" pad="7"/>
<connect gate="G$1" pin="VBAT" pad="1"/>
<connect gate="G$1" pin="VDD" pad="23 35 48"/>
<connect gate="G$1" pin="VDDA" pad="21"/>
<connect gate="G$1" pin="VREF+" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RFSW6042" prefix="IC">
<gates>
<gate name="G$1" symbol="RFSW6042"/>
</gates>
<devices>
<device name="" package="QFN40P180X180X55-13T76N">
<connects>
<connect gate="G$1" pin="ANT" pad="7"/>
<connect gate="G$1" pin="C1" pad="2"/>
<connect gate="G$1" pin="C2" pad="1"/>
<connect gate="G$1" pin="GND" pad="5 8 10 12 13"/>
<connect gate="G$1" pin="RF1" pad="9"/>
<connect gate="G$1" pin="RF2" pad="11"/>
<connect gate="G$1" pin="RF3" pad="6"/>
<connect gate="G$1" pin="RF4" pad="4"/>
<connect gate="G$1" pin="VDD" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MINI-USB-SCHIELD-" prefix="X">
<description>&lt;b&gt;MINI USB-B Conector&lt;/b&gt;&lt;p&gt;
Source: www.cypressindustries.com</description>
<gates>
<gate name="G$1" symbol="MINI-USB-5"/>
<gate name="S" symbol="SHIELD_4"/>
</gates>
<devices>
<device name="32005-301" package="32005-301">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="S" pin="S1" pad="M1"/>
<connect gate="S" pin="S2" pad="M2"/>
<connect gate="S" pin="S3" pad="M3"/>
<connect gate="S" pin="S4" pad="M4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STW81200" prefix="IC">
<gates>
<gate name="LDO" symbol="STW8100LDO"/>
<gate name="RF" symbol="STW81200RF"/>
<gate name="SUP" symbol="STW81200SUPPLY"/>
</gates>
<devices>
<device name="" package="QFN50P600X600X100-37T410N">
<connects>
<connect gate="LDO" pin="CBYP" pad="7"/>
<connect gate="LDO" pin="CBYP_4V5" pad="1"/>
<connect gate="LDO" pin="GND" pad="37"/>
<connect gate="LDO" pin="VIN_LDO_4V5" pad="36"/>
<connect gate="LDO" pin="VIN_LDO_REF" pad="18"/>
<connect gate="LDO" pin="VIN_LDO_RF_DIG" pad="28"/>
<connect gate="LDO" pin="VIN_LDO_VCO" pad="9"/>
<connect gate="LDO" pin="VR" pad="10"/>
<connect gate="LDO" pin="VREG_4V5" pad="2"/>
<connect gate="LDO" pin="VREG_DIG" pad="27"/>
<connect gate="LDO" pin="VREG_REF" pad="19"/>
<connect gate="LDO" pin="VREG_RF" pad="29"/>
<connect gate="LDO" pin="VREG_VCO" pad="8"/>
<connect gate="RF" pin="EXTVCO_INN" pad="13"/>
<connect gate="RF" pin="EXTVCO_INP" pad="12"/>
<connect gate="RF" pin="HW_PD" pad="4"/>
<connect gate="RF" pin="ICP" pad="15"/>
<connect gate="RF" pin="LD_SDO" pad="22"/>
<connect gate="RF" pin="LE" pad="25"/>
<connect gate="RF" pin="PD_RF1" pad="5"/>
<connect gate="RF" pin="PD_RF2/FL_SW" pad="6"/>
<connect gate="RF" pin="REF_CLKN" pad="20"/>
<connect gate="RF" pin="REF_CLKP" pad="21"/>
<connect gate="RF" pin="RF1_OUTN" pad="30"/>
<connect gate="RF" pin="RF1_OUTP" pad="31"/>
<connect gate="RF" pin="RF2_OUTN" pad="33"/>
<connect gate="RF" pin="RF2_OUTP" pad="34"/>
<connect gate="RF" pin="SCK" pad="24"/>
<connect gate="RF" pin="SDI" pad="23"/>
<connect gate="RF" pin="TEST_SE" pad="35"/>
<connect gate="RF" pin="VCTRL" pad="11"/>
<connect gate="SUP" pin="VCC_CPOUT" pad="16"/>
<connect gate="SUP" pin="VCC_RFOUT" pad="32"/>
<connect gate="SUP" pin="VCC_VCO_CORE" pad="3"/>
<connect gate="SUP" pin="VDD_CP" pad="14"/>
<connect gate="SUP" pin="VDD_DSM_NDIV" pad="26"/>
<connect gate="SUP" pin="VDD_PFD" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PJ-014D" prefix="J">
<gates>
<gate name="G$1" symbol="DC-JACK-SWITCH"/>
</gates>
<devices>
<device name="" package="PJ-014D">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP0603A" prefix="LP">
<gates>
<gate name="G$1" symbol="LOWPASS"/>
</gates>
<devices>
<device name="" package="FILTRDFN160X84X70-4N">
<connects>
<connect gate="G$1" pin="GND" pad="2 3"/>
<connect gate="G$1" pin="IN" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RFSA3714" prefix="IC">
<gates>
<gate name="G$1" symbol="F1958"/>
</gates>
<devices>
<device name="" package="QFN50P400X400X75-25T270">
<connects>
<connect gate="G$1" pin="CLK" pad="17"/>
<connect gate="G$1" pin="D0" pad="1"/>
<connect gate="G$1" pin="D1" pad="24"/>
<connect gate="G$1" pin="D2" pad="23"/>
<connect gate="G$1" pin="D3" pad="22"/>
<connect gate="G$1" pin="D4" pad="21"/>
<connect gate="G$1" pin="D5" pad="20"/>
<connect gate="G$1" pin="D6" pad="19"/>
<connect gate="G$1" pin="DATA" pad="18"/>
<connect gate="G$1" pin="GND" pad="4 6 7 8 9 10 11 12 13 15 25" route="any"/>
<connect gate="G$1" pin="LE" pad="16"/>
<connect gate="G$1" pin="MODE" pad="3"/>
<connect gate="G$1" pin="RF1" pad="5"/>
<connect gate="G$1" pin="RF2" pad="14"/>
<connect gate="G$1" pin="VDD" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SSM3J338R" prefix="Q">
<gates>
<gate name="G$1" symbol="P-MOSFET"/>
</gates>
<devices>
<device name="" package="SOTFL95P240X80-3N">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADL5801" prefix="IC">
<gates>
<gate name="G$1" symbol="ADL5801"/>
</gates>
<devices>
<device name="" package="QFN50P400X400X100-25T250N">
<connects>
<connect gate="G$1" pin="DETO" pad="11"/>
<connect gate="G$1" pin="ENBL" pad="9"/>
<connect gate="G$1" pin="GND" pad="1 2 5 6 8 12 14 17 19 23 25"/>
<connect gate="G$1" pin="IN+" pad="15"/>
<connect gate="G$1" pin="IN-" pad="16"/>
<connect gate="G$1" pin="LO+" pad="3"/>
<connect gate="G$1" pin="LO-" pad="4"/>
<connect gate="G$1" pin="OUT+" pad="20"/>
<connect gate="G$1" pin="OUT-" pad="21"/>
<connect gate="G$1" pin="VPDT" pad="13"/>
<connect gate="G$1" pin="VPLO" pad="7 24"/>
<connect gate="G$1" pin="VPRF" pad="18"/>
<connect gate="G$1" pin="VSET" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT5560" prefix="IC">
<gates>
<gate name="G$1" symbol="LT5560"/>
</gates>
<devices>
<device name="" package="SON50P300X300X80-9T165X238">
<connects>
<connect gate="G$1" pin="EN" pad="2"/>
<connect gate="G$1" pin="GND" pad="9"/>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="4"/>
<connect gate="G$1" pin="LO+" pad="8"/>
<connect gate="G$1" pin="LO-" pad="1"/>
<connect gate="G$1" pin="OUT+" pad="6"/>
<connect gate="G$1" pin="OUT-" pad="5"/>
<connect gate="G$1" pin="VCC" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X10" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINH2X10"/>
</gates>
<devices>
<device name="" package="2X10">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="19" pad="19"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="20" pad="20"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="C-EU" prefix="C" uservalue="yes">
<description>&lt;B&gt;CAPACITOR&lt;/B&gt;, European symbol</description>
<gates>
<gate name="G$1" symbol="C-EU"/>
</gates>
<devices>
<device name="C0603" package="C0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1206" package="C1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TE_2118718-2" prefix="SH">
<gates>
<gate name="G$1" symbol="SHIELD"/>
</gates>
<devices>
<device name="" package="TE_2118718-2">
<connects>
<connect gate="G$1" pin="GND" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AMPHENOL_901-10510-2" prefix="J">
<gates>
<gate name="G$1" symbol="BNC-FGND"/>
</gates>
<devices>
<device name="" package="AMPHENOL_901-10510-2">
<connects>
<connect gate="G$1" pin="1" pad="S"/>
<connect gate="G$1" pin="2" pad="G1 G2 G3 G4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BU-1420701851" prefix="J">
<gates>
<gate name="G$1" symbol="BNC-FGND"/>
</gates>
<devices>
<device name="" package="BU-1420701851">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="G@1 G@2 G@3 G@4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD9913" prefix="IC">
<gates>
<gate name="G$1" symbol="AD9913"/>
</gates>
<devices>
<device name="" package="QFN50P500X500X80-33T310">
<connects>
<connect gate="G$1" pin="#SER/PAR" pad="10"/>
<connect gate="G$1" pin="/CS" pad="28"/>
<connect gate="G$1" pin="/IOUT" pad="19"/>
<connect gate="G$1" pin="/REF_CLK" pad="14"/>
<connect gate="G$1" pin="ADR0/D0" pad="8"/>
<connect gate="G$1" pin="ADR1/D1" pad="7"/>
<connect gate="G$1" pin="ADR2/D2" pad="6"/>
<connect gate="G$1" pin="ADR6/D6" pad="32"/>
<connect gate="G$1" pin="ADR7/D7" pad="31"/>
<connect gate="G$1" pin="AGND" pad="11 15 18 21 23"/>
<connect gate="G$1" pin="AVDD" pad="12 16 17 22"/>
<connect gate="G$1" pin="DGND" pad="5"/>
<connect gate="G$1" pin="DVDD" pad="4"/>
<connect gate="G$1" pin="EP" pad="33"/>
<connect gate="G$1" pin="IOUT" pad="20"/>
<connect gate="G$1" pin="IO_UPDATE" pad="27"/>
<connect gate="G$1" pin="MASTER_RESET" pad="25"/>
<connect gate="G$1" pin="PS0/ADR3/D3" pad="3"/>
<connect gate="G$1" pin="PS1/ADR4/D4" pad="2"/>
<connect gate="G$1" pin="PS2/ADR5/D5" pad="1"/>
<connect gate="G$1" pin="PWR_DWN_CTL" pad="26"/>
<connect gate="G$1" pin="REF_CLK" pad="13"/>
<connect gate="G$1" pin="RSET" pad="24"/>
<connect gate="G$1" pin="SCLK" pad="30"/>
<connect gate="G$1" pin="SDIO" pad="29"/>
<connect gate="G$1" pin="SYNC_CLK" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SI5332A-GM1" prefix="IC">
<gates>
<gate name="G$1" symbol="SI5332A-GM1"/>
</gates>
<devices>
<device name="" package="QFN50P500X500X100-33T345N">
<connects>
<connect gate="G$1" pin="CLKIN_2" pad="2"/>
<connect gate="G$1" pin="CLKIN_2B" pad="3"/>
<connect gate="G$1" pin="GND" pad="33"/>
<connect gate="G$1" pin="INPUT1" pad="8"/>
<connect gate="G$1" pin="INPUT2" pad="17"/>
<connect gate="G$1" pin="INPUT3" pad="24"/>
<connect gate="G$1" pin="INPUT4" pad="28"/>
<connect gate="G$1" pin="INPUT5" pad="29"/>
<connect gate="G$1" pin="OUT0" pad="12"/>
<connect gate="G$1" pin="OUT0B" pad="11"/>
<connect gate="G$1" pin="OUT1" pad="15"/>
<connect gate="G$1" pin="OUT1B" pad="14"/>
<connect gate="G$1" pin="OUT2" pad="19"/>
<connect gate="G$1" pin="OUT2B" pad="18"/>
<connect gate="G$1" pin="OUT3" pad="22"/>
<connect gate="G$1" pin="OUT3B" pad="21"/>
<connect gate="G$1" pin="OUT4" pad="27"/>
<connect gate="G$1" pin="OUT4B" pad="26"/>
<connect gate="G$1" pin="OUT5" pad="31"/>
<connect gate="G$1" pin="OUT5B" pad="30"/>
<connect gate="G$1" pin="SCLK" pad="9"/>
<connect gate="G$1" pin="SDA" pad="10"/>
<connect gate="G$1" pin="VDDA" pad="7"/>
<connect gate="G$1" pin="VDDO0" pad="13"/>
<connect gate="G$1" pin="VDDO1" pad="16"/>
<connect gate="G$1" pin="VDDO2" pad="20"/>
<connect gate="G$1" pin="VDDO3" pad="23"/>
<connect gate="G$1" pin="VDDO4" pad="25"/>
<connect gate="G$1" pin="VDDO5" pad="32"/>
<connect gate="G$1" pin="VDD_DIG" pad="1"/>
<connect gate="G$1" pin="VDD_XTAL" pad="4"/>
<connect gate="G$1" pin="XA/CLKIN1" pad="5"/>
<connect gate="G$1" pin="XB" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L462CE" prefix="IC">
<gates>
<gate name="G$1" symbol="STM32L462CE"/>
</gates>
<devices>
<device name="" package="QFN50P700X700X60-49T560N">
<connects>
<connect gate="G$1" pin="EP" pad="49"/>
<connect gate="G$1" pin="NRST" pad="7"/>
<connect gate="G$1" pin="PA0" pad="10"/>
<connect gate="G$1" pin="PA1" pad="11"/>
<connect gate="G$1" pin="PA10" pad="31"/>
<connect gate="G$1" pin="PA11" pad="32"/>
<connect gate="G$1" pin="PA12" pad="33"/>
<connect gate="G$1" pin="PA13/SWDIO" pad="34"/>
<connect gate="G$1" pin="PA14/SWCLK" pad="37"/>
<connect gate="G$1" pin="PA15" pad="38"/>
<connect gate="G$1" pin="PA2" pad="12"/>
<connect gate="G$1" pin="PA3" pad="13"/>
<connect gate="G$1" pin="PA4" pad="14"/>
<connect gate="G$1" pin="PA5" pad="15"/>
<connect gate="G$1" pin="PA6" pad="16"/>
<connect gate="G$1" pin="PA7" pad="17"/>
<connect gate="G$1" pin="PA8" pad="29"/>
<connect gate="G$1" pin="PA9" pad="30"/>
<connect gate="G$1" pin="PB0" pad="18"/>
<connect gate="G$1" pin="PB1" pad="19"/>
<connect gate="G$1" pin="PB10" pad="21"/>
<connect gate="G$1" pin="PB11" pad="22"/>
<connect gate="G$1" pin="PB12" pad="25"/>
<connect gate="G$1" pin="PB13" pad="26"/>
<connect gate="G$1" pin="PB14" pad="27"/>
<connect gate="G$1" pin="PB15" pad="28"/>
<connect gate="G$1" pin="PB2" pad="20"/>
<connect gate="G$1" pin="PB3" pad="39"/>
<connect gate="G$1" pin="PB4" pad="40"/>
<connect gate="G$1" pin="PB5" pad="41"/>
<connect gate="G$1" pin="PB6" pad="42"/>
<connect gate="G$1" pin="PB7" pad="43"/>
<connect gate="G$1" pin="PB8" pad="45"/>
<connect gate="G$1" pin="PB9" pad="46"/>
<connect gate="G$1" pin="PC13" pad="2"/>
<connect gate="G$1" pin="PC14-OSC32_IN" pad="3"/>
<connect gate="G$1" pin="PC15-OSC32_OUT" pad="4"/>
<connect gate="G$1" pin="PH0-OSC_IN" pad="5"/>
<connect gate="G$1" pin="PH1_OSC_OUT" pad="6"/>
<connect gate="G$1" pin="PH3-BOOT0" pad="44"/>
<connect gate="G$1" pin="VBAT" pad="1"/>
<connect gate="G$1" pin="VDD" pad="24 48"/>
<connect gate="G$1" pin="VDDA/VREF+" pad="9"/>
<connect gate="G$1" pin="VDDUSB" pad="36"/>
<connect gate="G$1" pin="VSS" pad="23 35 47"/>
<connect gate="G$1" pin="VSSA/VREF-" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PAT0816-C-3DB-T5" prefix="R">
<description>3dB pad attenuator</description>
<gates>
<gate name="G$1" symbol="ATTENUATOR_3PIN"/>
</gates>
<devices>
<device name="" package="PAT0816">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
