<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="100" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0" x2="50" y2="0" width="0" layer="20"/>
<wire x1="50" y1="0" x2="50" y2="100" width="0" layer="20"/>
<wire x1="50" y1="100" x2="0" y2="100" width="0" layer="20"/>
<text>2.6mm</text>
<text>2.4mm</text>
<text>2.2mm</text>
<text>2.0mm</text>
<text>1.8mm</text>
<text>GND cutout size variation</text>
<text>RLB Test</text>
<text>out+</text>
<text>out-</text>
<text>DUT</text>
<text>Source</text>
<text>Microstrip</text>
<text>Coplanar Waveguide</text>
</plain>
<libraries>
<library name="VNA">
<description>Generated from &lt;b&gt;VNA.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="AMPHENOL_132289">
</package>
<package name="R0402">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="EASTEVER_BALUN">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="VNA" package="AMPHENOL_132289" value="AMPHENOL_132289">
<attribute name="VALUE"/>
</element>
<element name="J2" library="VNA" package="AMPHENOL_132289" value="AMPHENOL_132289">
<attribute name="VALUE"/>
</element>
<element name="J3" library="VNA" package="AMPHENOL_132289" value="AMPHENOL_132289">
<attribute name="VALUE"/>
</element>
<element name="J4" library="VNA" package="AMPHENOL_132289" value="AMPHENOL_132289">
<attribute name="VALUE"/>
</element>
<element name="J5" library="VNA" package="AMPHENOL_132289" value="AMPHENOL_132289">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J6" library="VNA" package="AMPHENOL_132289" value="AMPHENOL_132289">
<attribute name="VALUE"/>
</element>
<element name="J7" library="VNA" package="AMPHENOL_132289" value="AMPHENOL_132289">
<attribute name="VALUE"/>
</element>
<element name="J8" library="VNA" package="AMPHENOL_132289" value="AMPHENOL_132289">
<attribute name="VALUE"/>
</element>
<element name="J9" library="VNA" package="AMPHENOL_132289" value="AMPHENOL_132289">
<attribute name="VALUE"/>
</element>
<element name="R1" library="VNA" package="R0402" value="49R9">
<attribute name="VALUE"/>
</element>
<element name="R2" library="VNA" package="R0402" value="49R9">
<attribute name="VALUE"/>
</element>
<element name="R3" library="VNA" package="R0402" value="49R9">
<attribute name="VALUE"/>
</element>
<element name="R4" library="VNA" package="R0402" value="49R9">
<attribute name="VALUE"/>
</element>
<element name="R5" library="VNA" package="R0402" value="49R9">
<attribute name="VALUE"/>
</element>
<element name="T1" library="VNA" package="EASTEVER_BALUN" value="B012-617DB-1-63-B331">
<attribute name="VALUE"/>
</element>
<element name="J10" library="VNA" package="AMPHENOL_132289" value="AMPHENOL_132289">
<attribute name="VALUE"/>
</element>
<element name="J11" library="VNA" package="AMPHENOL_132289" value="AMPHENOL_132289">
<attribute name="VALUE"/>
</element>
<element name="J12" library="VNA" package="AMPHENOL_132289" value="AMPHENOL_132289">
<attribute name="VALUE"/>
</element>
<element name="R6" library="VNA" package="R0402" value="49R9">
<attribute name="VALUE"/>
</element>
<element name="R7" library="VNA" package="R0402" value="49R9">
<attribute name="VALUE"/>
</element>
<element name="R8" library="VNA" package="R0402" value="49R9">
<attribute name="VALUE"/>
</element>
<element name="J13" library="VNA" package="AMPHENOL_132289" value="AMPHENOL_132289">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="R1" pad="1"/>
<contactref element="J1" pad="G@1"/>
<contactref element="J1" pad="G@2"/>
<contactref element="J1" pad="G@3"/>
<contactref element="J1" pad="G@4"/>
<contactref element="R2" pad="1"/>
<contactref element="J2" pad="G@1"/>
<contactref element="J2" pad="G@2"/>
<contactref element="J2" pad="G@3"/>
<contactref element="J2" pad="G@4"/>
<contactref element="R3" pad="1"/>
<contactref element="J3" pad="G@1"/>
<contactref element="J3" pad="G@2"/>
<contactref element="J3" pad="G@3"/>
<contactref element="J3" pad="G@4"/>
<contactref element="R4" pad="1"/>
<contactref element="J4" pad="G@1"/>
<contactref element="J4" pad="G@2"/>
<contactref element="J4" pad="G@3"/>
<contactref element="J4" pad="G@4"/>
<contactref element="R5" pad="1"/>
<contactref element="J5" pad="G@1"/>
<contactref element="J5" pad="G@2"/>
<contactref element="J5" pad="G@3"/>
<contactref element="J5" pad="G@4"/>
<contactref element="J6" pad="G@1"/>
<contactref element="J6" pad="G@2"/>
<contactref element="J6" pad="G@3"/>
<contactref element="J6" pad="G@4"/>
<contactref element="J7" pad="G@1"/>
<contactref element="J7" pad="G@2"/>
<contactref element="J7" pad="G@3"/>
<contactref element="J7" pad="G@4"/>
<contactref element="J8" pad="G@1"/>
<contactref element="J8" pad="G@2"/>
<contactref element="J8" pad="G@3"/>
<contactref element="J8" pad="G@4"/>
<contactref element="J9" pad="G@1"/>
<contactref element="J9" pad="G@2"/>
<contactref element="J9" pad="G@3"/>
<contactref element="J9" pad="G@4"/>
<contactref element="J12" pad="G@1"/>
<contactref element="J12" pad="G@4"/>
<contactref element="J12" pad="G@3"/>
<contactref element="J12" pad="G@2"/>
<contactref element="J11" pad="G@1"/>
<contactref element="J11" pad="G@4"/>
<contactref element="J11" pad="G@3"/>
<contactref element="J11" pad="G@2"/>
<contactref element="R6" pad="1"/>
<contactref element="J10" pad="G@1"/>
<contactref element="J10" pad="G@4"/>
<contactref element="J10" pad="G@3"/>
<contactref element="J10" pad="G@2"/>
<contactref element="J13" pad="G@1"/>
<contactref element="J13" pad="G@4"/>
<contactref element="J13" pad="G@3"/>
<contactref element="J13" pad="G@2"/>
</signal>
<signal name="N$1">
<contactref element="J1" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="J2" pad="1"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="J3" pad="1"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="J4" pad="1"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="J5" pad="1"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="J6" pad="1"/>
<contactref element="J7" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="J8" pad="1"/>
<contactref element="J9" pad="1"/>
</signal>
<signal name="CUTOUT">
</signal>
<signal name="N$9">
<contactref element="J12" pad="1"/>
<contactref element="T1" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="R8" pad="2"/>
<contactref element="J10" pad="1"/>
<contactref element="T1" pad="6"/>
</signal>
<signal name="N$11">
<contactref element="R7" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="T1" pad="4"/>
</signal>
<signal name="N$12">
<contactref element="J13" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="T1" pad="2"/>
<contactref element="J11" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
